| Español |

Products List

- Anchorge System
  - Anchor Head
  - Anchor Plate
  - Oil Jack & Pump
  - Wedge (Grip)
- Hot-Dipped Galvanized Steel Strand
- Hot-Dipped Galvanized Steel Wire
- Prestressing Strand
  - Filled Epoxy-Coated Seven-Wire Prestressing Steel Strand
  - High-Tensile Prestressing Hot-dipped Galvanized Steel Strand
  - Low Relaxation Prestressed Concrete Steel Strand
  - Retarded Bonded Prestressing Steel Strand
  - Unbonded Prestressing Steel Strand
- Prestressed Concrete Steel Bar
- Prestressing Wire
  - High-Tensile Prestressing Hot-Dipped Galvanized Steel Wire
  - Prestressed Concrete Wire
- Zinc-5%Al Coated (Galfan) Steel Strand
- Zn-5% Al Coated Steel Wire

Home -> Prestressing Wire -> Prestressed Concrete WireProducts

## Prestressed Concrete Wire

Apllication: Pre-tension and post-tension concrete products such as railway sleeper, electrical poles,and hollow-core floor block,civil engineering construction of large scale railroad,highway bridges buildings trusses,overhead crane beams,industrial prefabricated concrete floor,wall board,tubular piles,TV towers and nuclear power station,etc.
Features: High tensile strength,Low relaxation,Straight,stable modulus of elasticity,non-joints,little residual stress
Diameter: 4mm / 5mm / 6mm / 7mm / 9mm
Inner diameter of coil: 1700mm
Outer diameter of coil: 2200mm
Coil Weight： 1.0-3.0MT
Standard: GB/T5223-2002, ASTM A421, BS5896, JIS G3536, AS/NZS4672.1:2007
Tensile strength: 1470Mpa / 1570Mpa / 1670Mp

- Prestressing Wire 01
- Prestressing Wire 02
- Prestressing Wire 03
- Prestressing Wire 04
- Prestressing Wire 05