| Español |

Products List

- Anchorge System
  - Anchor Head
  - Anchor Plate
  - Oil Jack & Pump
  - Wedge (Grip)
- Hot-Dipped Galvanized Steel Strand
- Hot-Dipped Galvanized Steel Wire
- Prestressing Strand
  - Filled Epoxy-Coated Seven-Wire Prestressing Steel Strand
  - High-Tensile Prestressing Hot-dipped Galvanized Steel Strand
  - Low Relaxation Prestressed Concrete Steel Strand
  - Retarded Bonded Prestressing Steel Strand
  - Unbonded Prestressing Steel Strand
- Prestressed Concrete Steel Bar
- Prestressing Wire
  - High-Tensile Prestressing Hot-Dipped Galvanized Steel Wire
  - Prestressed Concrete Wire
- Zinc-5%Al Coated (Galfan) Steel Strand
- Zn-5% Al Coated Steel Wire

Home -> Prestressing Strand -> Filled Epoxy-Coated Seven-Wire Prestressing Steel StrandProducts

## Filled Epoxy-Coated Seven-Wire Prestressing Steel Strand

Application: Cables of cable-stayed bridges and external reinforcing cables of various prestressed structures（non-exposure in the concrete mortar).
Features: High tensile strength, low relaxation, stable modulus of elasticity, non-joint gauge, little residual stress, good corrosion resistance.
Structure and Diameter:
1x7, Dia 12.5mm / 12.9mm / 15.2mm / 15.7mm
Standard: Chinese standard GB/T 25823-2010, ASTM A882
Coating Thickness：0.38-1.14mm
Packing: Steel strips bundled and plastic sheets wrapped outside.
Mechanical property is same as normal prestressing strand.

- Filled Epoxy-Coated Seven-Wire Prestressing Steel Strand 01
- Filled Epoxy-Coated Seven-Wire Prestressing Steel Strand 02
- Filled Epoxy-Coated Seven-Wire Prestressing Steel Strand 03
- Filled Epoxy-Coated Seven-Wire Prestressing Steel Strand 04