| English |

| hkwins@hebwl.com

Lista de productos

- Anchorge System
  - Cabeza del ancla
  - Placa de anclaje
  - Oil Jack & Pump
  - Cuña (agarre)
- Filamento de acero galvanizado en caliente
- Alambre de acero galvanizado en caliente
- Prestressing Strand
  - Filamento de acero pretensado con recubrimiento epóxico de siete alambres
  - Filamento de acero pretensado de alta resistencia a la tracción galvanizado en caliente
  - Filamento de acero de hormigón pretensado de baja relajación
  - Filamento de acero pretensado de unión lenta
  - Filamento de acero pretensado sin unión
- Prestressed Concrete Steel Bar
- Prestressing Wire
  - High-Tensile Prestressing Hot-Dipped Galvanized Steel Wire
  - Prestressed Concrete Wire
- Zinc-5%Al Coated (Galfan) Steel Strand
- Zn-5% Al Coated Steel Wire

Home -> Prestressing Wire -> High-Tensile Prestressing Hot-Dipped Galvanized Steel WireProductos

## High-Tensile Prestressing Hot-Dipped Galvanized Steel Wire

Application:Main cables of long-span suspension bridges and cables of cable-stayed bridges.
Features: High tensile strength, low relaxation, stable modulus of elasticity, non-joint, little residual stress, good corrosion resistance for post-galvanized surface.
Diameter: 5mm / 7mm
Standard: Chinese standard GB/T17101-2008, French standard NF A35-035-2001
Packing: Steel strips bundled and plastic sheets wrapped outside.

- High-Tensile Prestressing Hot-Dipped Galvanized Steel Wire 01
- High-Tensile Prestressing Hot-Dipped Galvanized Steel Wire 02
- High-Tensile Prestressing Hot-Dipped Galvanized Steel Wire 03
- High-Tensile Prestressing Hot-Dipped Galvanized Steel Wire 04
- High-Tensile Prestressing Hot-Dipped Galvanized Steel Wire 05