| Español |

Products List

- Anchorge System
  - Anchor Head
  - Anchor Plate
  - Oil Jack & Pump
  - Wedge (Grip)
- Hot-Dipped Galvanized Steel Strand
- Hot-Dipped Galvanized Steel Wire
- Prestressing Strand
  - Filled Epoxy-Coated Seven-Wire Prestressing Steel Strand
  - High-Tensile Prestressing Hot-dipped Galvanized Steel Strand
  - Low Relaxation Prestressed Concrete Steel Strand
  - Retarded Bonded Prestressing Steel Strand
  - Unbonded Prestressing Steel Strand
- Prestressed Concrete Steel Bar
- Prestressing Wire
  - High-Tensile Prestressing Hot-Dipped Galvanized Steel Wire
  - Prestressed Concrete Wire
- Zinc-5%Al Coated (Galfan) Steel Strand
- Zn-5% Al Coated Steel Wire

Home -> Hot-Dipped Galvanized Steel WireProducts

## Hot-Dipped Galvanized Steel Wire

Application: Steel core wire for ACSR, Power cable, Overhead conductors, Telecommunication cable, Messenger wire, Earth wire, Stay wire, Guy wire, Fence etc.
Structure and Diameter:
Dia 1.80～7.00mm
Standard: ASTM B498,EN50189,ICE888,BS4565.Other strandard as per customer's requirement.
Special specification and requirement may be ordered.
Packing: Steel strips bundled and plastic sheets wrapped outside.

- Hot-Dipped Galvanized Steel Wire 01
- Hot-Dipped Galvanized Steel Wire 02
- Hot-Dipped Galvanized Steel Wire 03
- Hot-Dipped Galvanized Steel Wire 04
- Hot-Dipped Galvanized Steel Wire 05
- Hot-Dipped Galvanized Steel Wire 06

Nominal diameter | Strength Grade
mm | Mpa
1 | 1270 | 1370 | 1470 | 1570 | 1670
1.1
1.2
1.3
1.4
1.5
1.6
1.7
1.8
2
2.2
2.4
2.6
2.8
3
3.2
3.5
3.8
4

Nominal diameter | Zn-coat thickness/(g/m2) ≥
mm | A | B | C
1 | 110 | 160 | -
1.2 | 110 | 160 | -
1.4 | 130 | 160 | -
1.6 | 130 | 180 | -
1.8 | 160 | 180 | -
2 | 200 | 200 | 230
2.3 | 200 | 200 | 250
2.6 | 230 | 230 | 260
2.9 | 230 | 250 | 280
3.2 | 230 | 275 | 300
3.5 | 250 | 275 | 320
3.8 | 250 | 275 | 330
4 | 250 | 300 | 350