| English |

| hkwins@hebwl.com

Lista de productos

- Anchorge System
  - Anchor Head
  - Anchor Plate
  - Oil Jack & Pump
  - Wedge (Grip)
- Hot-Dipped Galvanized Steel Strand
- Hot-Dipped Galvanized Steel Wire
- Prestressing Strand
  - Filled Epoxy-Coated Seven-Wire Prestressing Steel Strand
  - High-Tensile Prestressing Hot-dipped Galvanized Steel Strand
  - Low Relaxation Prestressed Concrete Steel Strand
  - Retarded Bonded Prestressing Steel Strand
  - Unbonded Prestressing Steel Strand
- Prestressed Concrete Steel Bar
- Prestressing Wire
  - High-Tensile Prestressing Hot-Dipped Galvanized Steel Wire
  - Prestressed Concrete Wire
- Zinc-5%Al Coated (Galfan) Steel Strand
- Zn-5% Al Coated Steel Wire

Home -> Prestressing Strand -> Low Relaxation Prestressed Concrete Steel StrandProductos

## Low Relaxation Prestressed Concrete Steel Strand

Application:Mainly used for prestressed concrete structural reinforcement, such as span railway and highway bridges, crane beam, ground anchoring project, multi-storey industrial plants,stadiums, water control projects, mines, nuclear power stations,etc.
Features: High tensile strength, low relaxation, stable modulus of elasticity, stress-relieved, straight, firm connection with concrete.
Structure and Diameter:
1x2 - Dia 5.0mm～12.0mm
1x3 - Dia 6.2mm～12.9mm
1x7 - Dia 9.53mm～21.6mm
1x19 - Dia 17.8mm～28.6mm
Outer diameter of coil: 1250mm
Inner diameter of coil: 750mm
Width of coil: 750mm
Coil Weight: 2.5-3.5MT
Standard:GB/T5224-2014,ASTM A416-2012,BS 5896,NBR 7483, JIS G3536-1999, AS/NZS4672.1:2007
Tensile Strength Grade:1570Mpa / 1670Mpa / 1720Mpa / 1770Mpa / 1860Mpa / 1900Mpa / 2100Mpa

- Low Relaxation Prestressed Concrete Steel Strand 01
- Low Relaxation Prestressed Concrete Steel Strand 02
- Low Relaxation Prestressed Concrete Steel Strand 03
- Low Relaxation Prestressed Concrete Steel Strand 04
- Low Relaxation Prestressed Concrete Steel Strand 05
- Low Relaxation Prestressed Concrete Steel Strand 06
- Low Relaxation Prestressed Concrete Steel Strand 07