| Español |

Products List

- Anchorge System
  - Anchor Head
  - Anchor Plate
  - Oil Jack & Pump
  - Wedge (Grip)
- Hot-Dipped Galvanized Steel Strand
- Hot-Dipped Galvanized Steel Wire
- Prestressing Strand
  - Filled Epoxy-Coated Seven-Wire Prestressing Steel Strand
  - High-Tensile Prestressing Hot-dipped Galvanized Steel Strand
  - Low Relaxation Prestressed Concrete Steel Strand
  - Retarded Bonded Prestressing Steel Strand
  - Unbonded Prestressing Steel Strand
- Prestressed Concrete Steel Bar
- Prestressing Wire
  - High-Tensile Prestressing Hot-Dipped Galvanized Steel Wire
  - Prestressed Concrete Wire
- Zinc-5%Al Coated (Galfan) Steel Strand
- Zn-5% Al Coated Steel Wire

Home -> Anchorge System -> Anchor HeadProducts

## Anchor Head

Application: Used in pre-tension or post-tension for concrete constructions as building materials. lock the steel strand wires on/under clases of 2000MPa standard strength, which is usually in diameters of 12.7mm\12.9mm\15.2mm\15.7mm.
Quality of steel: 40Cr
Hardness: HRC1-32
Anchorage efficiency factor : ≥ 0.95
Elongation of prestressing steel on free length of tendon at ultimate force: ≥ 2.0%

- Anchor Head 10
- Anchor Head 11
- Anchor Head 12
- 01

2
1

1. Type:KM series, M5-M22 |  |
2. Shape: round and flat , from 1 hole to 55holes
3. Application: prestressing works usage |
4. Standard: ASTM/BS/JIS/GB/AS |
5. Model type for PC strand: |  |

Model# | PC Strand Size
M5,M6,M7 | 7.0mm, 6.0mm, 5.0mm spiral ribbed pc wire
M10 | 9.3mm, 9.53mm pc strand;
M11 | 10.8mm pc strand
M13 | 12.7mm, 12.5mm & 12.9mm pc strand
M15 | 15.2 or 15.24mm, 15.7mm
M18 | 17.8mm pc strand
M22 | 21.6/21.8mm pc strand

6.Packing: In box or wood carton