| Español |

Products List

- Anchorge System
  - Anchor Head
  - Anchor Plate
  - Oil Jack & Pump
  - Wedge (Grip)
- Hot-Dipped Galvanized Steel Strand
- Hot-Dipped Galvanized Steel Wire
- Prestressing Strand
  - Filled Epoxy-Coated Seven-Wire Prestressing Steel Strand
  - High-Tensile Prestressing Hot-dipped Galvanized Steel Strand
  - Low Relaxation Prestressed Concrete Steel Strand
  - Retarded Bonded Prestressing Steel Strand
  - Unbonded Prestressing Steel Strand
- Prestressed Concrete Steel Bar
- Prestressing Wire
  - High-Tensile Prestressing Hot-Dipped Galvanized Steel Wire
  - Prestressed Concrete Wire
- Zinc-5%Al Coated (Galfan) Steel Strand
- Zn-5% Al Coated Steel Wire

Home -> Zn-5% Al Coated Steel WireProducts

## Zn-5% Al Coated Steel Wire

Application: Steel core wire for ACSR, Power cable, Overhead conductors, Telecommunication cable, Messenger wire, Earth wire, Stay wire, Guy wire, Fence etc.
Structure and Diameter:
Dia 1.80～7.00mm
Standard: GB/T20492-2006.Other strandard as per customer's requirement.
Special specification and requirement may be ordered.
Packing: Steel strips bundled and plastic sheets wrapped outside.

- Zn-5% Al Coated Steel Wire 01
- Zn-5% Al Coated Steel Wire 02
- Zn-5% Al Coated Steel Wire 03
- Zn-5% Al Coated Steel Wire 04
- Zn-5% Al Coated Steel Wire 05

Nominal diameter | Zn-coat thickness/(g/m2) ≥
mm | A | B | C
>1.24～1.50 | 185 | 370 | 555
>1.50～1.75 | 200 | 400 | 600
>1.75～2.25 | 215 | 430 | 645
>2.25～3.00 | 230 | 460 | 690
>3.00～3.50 | 245 | 490 | 735
>3.50～4.25 | 260 | 520 | 780
>4.25～4.75 | 275 | 550 | 825
>4.75～5.50 | 290 | 580 | 870