| Welcome to HEBEI XIAOPENG !

| English |  | русский |  | Português |
E-maill: admin@hoistcn.com

Products List
Contact Us

| Taocheng Development Zone, Hengshui City, Hebei Province. China
| +86-318-5111881
| +86-318-5111551
| admin@hoistcn.com ktxfactory@163.com

Home -> CD1 Electric Wire Rope HoistProducts

# CD1 Electric wire rope hoist

<<Previous Next>>

Details Show

Details

CD1 electric wire rope hoist are kinds of light small its heavy equipment, has the structure to be compact, the weight is light, the volume is small, the spare part versatility is strong, operation simple and so on merits. The reduction gear uses the hard tooth face rotation design, the life is long, the mechanical efficiency is high. The electrical machinery uses the cone-shape rotor to apply the brake electrically operated several, has the high and low bidirectional security stop block.

>The lifting motor of our electric wire rope hoist is Nanjing special motor ,the best quality motor from China.

> For rope guide, our electric hoist is not the original one, the original one is easy to be broken; the new type is with pressure lever and pressure wheel, the lever could press wire rope, and the wheel only allow one wire rope go out, it would avoid the wire rope goes wrong!

> The hook of our electric wire rope hoist is special, it is very beautiful, the quality is also very good.

> The gear of gear box is the best quality gear in China, the material of first axle and first gear is 40Cr, the other axles and gears are with high frequency quenching, it guarantee the gears wearing resistance.

> The shaft joint is large open shaft, there is the spline in it, it is better buffered the force when the motor start and stop, it make the axle and jackshaft more resistant. It reduce wear of central axle and jackshaft.

> The gear box of our electric wire rope hoist cover adopted the casing of automotive technology, makes paint more bright and delicate.

> Our electric wire rope hoist is with load limiter.

Techanical Data

Model | CD1 0.5T | CD1 1T | CD1 2T | CD1 3T | CD1 5T | CD1 10T | CD1 16T | CD1 20T | CD1 25T | CD1 32T
Capacity (t) | 0.5 | 1 | 2 | 3 | 5 | 10 | 16 | 20 | 25 | 32
Standard lifting height (m) | 6-12 | 6-30 | 6-30 | 6-30 | 6-30 | 9-30 | 9-18 | 9-18 | 9-24 | 9-24
Lifting speed (m/min) | 8 | 8 | 8 | 8 | 8 | 7 | 3.5 | 3.5 | 2.4 | 2.4
Running speed (m/min) | 20 | 20 | 20 | 20 | 20 | 20 | 20 | 20 | 20 | -
Wire rope type | D-6X37+1 | D-6X37+1 | D-6X37+1 | D-6X37+1 | D-6X37+1 | D-6X37+1 | D-6X37+1 | D-6X37+1 | D-6X37+1 | D-6X19+1
I-beam track type | 16-28b | 16-28b | 20a-32c | 20a-32c | 25a-63c | 25a-63c | 45a-63c | 50a-63c | 50a-63c | 50a-63c
Min. radius of curve (m) | 1.5 | 1.5-4 | 2-4 | 2-4 | 2.5-5 | 2.5-9 | 3-4.6 | 3-4.6 | 3-4.6 |
Power supply | 220V-440V,50/60HZ,3P
Working duty | Mid M3 | Mid M3 | Mid M3 | Mid M3 | Mid M3 | Mid M3 | Mid M2 | Mid M2 | Light M6 | Light M3

<<Previous Next>>
PRODUCT CATEGORY
GET IN TOUCH
HEBEI XIAOPENG HOISTING EQUIPMENT FACTORY
Address: Taocheng Development Zone, Hengshui City, Hebei Province. China.
Tel: +86-318-5111881
Fax: +86-318-5111551
Email: admin@hoistcn.com ktxfactory@163.com
Postcode: 053000
CONNECT WITH US

© 2016 HEBEI XIAOPENG HOISTING EQUIPMENT FACTORY | All Rights Reserved.