###
Products

# KT-560

- Previous

Description

320×240 TFT color screen

Measure mode: (P-E) pulse-echo and (E-E) thru-paint

A scan and B scan

Auto probe zero calibration

Auto probe indentify

Measuring range: T-E 0.65-400.0mm E-E 3.00-25.0mm

Option in Gain, Gate and Blank setting

Standard 5.0MHz transducer included, optional transducers

Display resolution 0.01mm/ 0.001in

Memory of 10000 readings in 100 files

USB output, easily works with A any Windows operating system 32bit and 64 bit.

Multiple languages support

2 year warranty

Physical

Operating Temperature:

-10℃ to 50 ℃ (-14℉to662℉)

Keyboard :

Membrane switch with 8 tactile

Keys

Case : ABS plastic

Data Output :

USB port ; Data output directly

Without any driver

Display: 320×240 TFT color display

Weight: 260g

Size:133L×75W×29H mm

(5.2L×3.0W×1.1H inch)

Ultrasonic Specifications

Measurement Modes:

Transmit-Echo

Echo-Echo (Thru-paint)

Receiver:

Manual or Auto gain control with 50dB range, depending on mode selected.

Display

Display Views:

Large Digits: Standard thickness view

B-Scan:

Scan Bar: Thickness 10 readings per second; Viewable in B-Scan and large Digit Views.

Power Source

Two 1.5V AA alkaline. Typically operates for 24 hours.

Measuring

Transmit-Echo Mode:

Measures from 0.65 to 400.0mm (0.025 to 15.748 inches)

Echo-Echo Mode: (Thru Paint & Coatings)

Measures from 3.00-25.0mm (0.118 to 1.000 inch). Range will

vary +/- depending on the thickness of coating.

Resolution: +/-0.01mm (0.001 inches)

Velocity Range:

1000 to 9999 meters/sec

.492 to .3936 inches/ms

Units: Metric & English

Transducer

Transducer Types:

Dual Element (2 to 10 MHz) with cable length 1.25m.

Custom transducers and cable lengths are available for special applications.

Transducer

Transducer Types:

Dual Element (2 to 10 MHz) with cable length 1.25m.

Custom transducers and cable lengths are available for special applications.

Memory

Data Structure:

English letter +Alpha numeric

Cell Contents:

10,000 readings,

Memory: build-in TIF card (8Gb)

Features

Gain, Gate and Blank:

Adjustable

Standard Mode: For general purpose.

Minimum Mode: Only the minimum value is shown during testing.

Difference Mode: The accurate differential value between measured value and reference value is shown.

Average Mode: The average value of 2-9 testing points is displayed.

Limit Mode:

Set Hi and Lo tolerances with audible beeper and visual LEDs.

Certification

Factory calibration traceable to JJF 1126-2004.

Warranty

2 years and repair for whole life

Big Digit View B-Scan View

Related Products

##### KT-6 / KT-7 ( E-E )

##### KT-360

##### KT-400

##### KT-500/500D/500DL

##### KT-300D / 310D

##### KT-300 / 310

- Previous

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.