###
Products

# AT60S

- Previous

Description

Thermal Imaging Cameras

AT60S are with ergonomic design, high performance with 5MP visual camera, interchangeable lens, large 5” foldable and rotatable LCD, manual & auto focus. They can provide powerful assistance for thermographers to have the most efficient instrument for maintenance inspections.

Have a wide range temperature measurement to satisfy variety of thermograph applications and they enable you to identify the small temperature difference that could cause big problems.

Features

Folding and 270° rotatable touch display
Auto/Motor focus for one-hand operation
Bright LED light, laser pointer
Built-in digital camera, 5.0M resolutions
Real-time thermal video transfer to PC via USB, and remote transfer via MSN and Skype
Dual image enhancement with visual - DEV . similar MSX.

Applications

Building Diagnostics
Electrical/Mechanical Inspection
Research & Development
Automation Applications
Preventative & Predictive Maintenance

Technical Specifications

Item | AT60S
Type | Uncooled FPA
IR resolution | 640×480
Pixel pitch | 17μm
Spectral range | 7.5～14μm
NETD/Sensitivity | 40mK
FOV | 24°×18°
Minimum imaging distance | 0.3m
IFOV | 0.68mrad
Focus | Auto/Motor/Manual
Lens(optional) | 45°×33°/0.5m、12°×9°/1m、6.2°×4.7°/8m
Display | 5”, 270° rotatable touch LCD, 800×480 pixels
Visual camera | 5.0 mega pixel
Frequency | 50Hz/60Hz
Zoom | 1X～8X continuous
Color palletes | 12 palletes(including iron, rainbow, white hot and black hot etc.)
Contrast/brightness | Auto/Manual
Temperature range | -20℃～+600℃(can be extended to 1200℃)
Temperature accuracy | ±2℃/±2%(reading)
Spotmeter | 10 adjustable spots
Line profile | Vertical/Horizontal
Area | 10 adjustable spots, 5 rectangle/circle boxes with max./min./avg temperature value
Isotherms analysis | Capture high/low temperature/interval
Alarm | Voice, color
Dew point alarm | Yes
Measurement correction | Auto/Manual
Emissivity correction | Adjustable from 0.01 to 1.0 or selected from list of materials
Background temperature correction | Auto
Atmospheric transmissivity correction | Auto
Setting function | Date/time, temperature unit ℃/℉/K, language
Video | Can be recorded and saved
Storage type | 64G SD card, >38400 images
Storage mode | Store signal frame image auto/manual
Signal frame infrared image format | JPEG, with 14-Bit measured data image
Signal frame visible light image format | JPEG or stored with signal frame image
Voice annotation | 60s voice record, stored with per image via built-in microphone
Laser Point
Grade/Type | Class 2, 1mW/635nm Red
Power interface | Yes
SD card slot | Yes
Video output | CVBS
Audio output | Yes
USB | Radiometric images transfer to and from PC
Tripod | 1/4” -20
Battery type | Lithium battery
Battery operation time | 3h continuous
External power | DC: 10V～15V
Charging system | Intelligent charger or in camera(AC adapter or 12V car charger)
Power saving | Yes
Operation temperature range | -20℃～+50℃
Storage temperature range | -40℃～+70℃
Humidity | ≤95%(Non-condense)
Shock | 2G(IEC60068-2-6)
Vibration | 25G(IEC60068-2-29)
Encapsulation | IP54(IEC60529)
Size | 215mm×145mm×135mm
Weight | ≤1.6kg(with battery and standard lens)
Standard | Thermal imaging camera with standard lens, 2 lithium batteries, battery charger, adapter, USB cable, SD card, card reader, software CD, warranty card, calibration certificate

Related Products

##### ATB6

##### ATH1

##### AT5X

##### AT15 & AT35

##### AT4 & AT8

##### AT3 / AT7

- Previous

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.