###
Products

# KT-350

- Previous
- Next

Description

FEATURES:

HIGH ACCURACY AND RESOLUTION UP TO 0.001mm or 0.0001 inch

MEASURING ULTRA THIN SAMPLE AS LOW AS 0.15mm or 0.006 inch

DISPLAY UNITS : IMPERIAL and METRIC

AUTOMATIC SELF CALIBRATION

COUPLANT INDICATOR

AUTOMATIC POWER OFF DEVICE

HIGH-LOW LIMIT ALARM

LCD BRIGHTNESS ADJUST

LOW BATTERY INDICTOR

TECHNICAL SPECIFICATIONS:

Measuring Range (for steel) | Interface-Echo Mode: (I-E or Standard Mode) | 1.50mm – 20.0mm (0.059in – 0.787 in)
Echo-Echo Mode: (E-E or High Precision Mode) | 0.15mm – 10.0mm (0.006in – 0.394in)
Measuring Accuracy | ±0.005mm or 0.0002 inch (if thickness < 3mm)
±0.05mm or 0.002 inch (if thickness < 20mm)
Display Resolution | mm : 0.1 / 0.01 / 0.001
inch : 0.01 / 0.001 / 0.0001
Sound Velocity Range | 1000 to 9999 m/sec (0.0394 – 0.3936 inch/ms)
Measuring Refresh Frequency | 4Hz in normal mode, up to 25Hz
Memory Capacity | 500 test values
Multiple Calibrations | One point or Two Point
Display LCD | 42×57mm LCD size with EI backlight and adjustable contrast, font size up to 13.75mm (0.54 inch)
Power Source | 2 pcs. 1.5v AA size batteries
Continuous working period | About 200 hours (with backlight off)
Power off | Auto power off if idle for 4 minutes
Operating Temperature | -10 °C to +50 °C
Unit Size | 2.9 W x 5.9 H x 1.26 D inches (73 W x 149 H x 32 D mm).
Weight | 200g

STANDARD DELIVERY:

Main Processor with Calibration block (4.00 mm)

Precision Probe with Replaceable Delay Tip

Coupling Paste

Operation Manual

Consumer-Type 2 AA Type Alkaline Battery (3 Volt)

Carrying Case

Related Products

##### KT-100D/200D

##### KT-100B/200B

##### KT-300 / 310

##### KT-300D / 310D

##### KT-500/500D/500DL

##### KT-560

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.