###
Products

# KFD-55

- Previous

Description

Water-proof Dust-proof Lightweight Hi-Bright Battery Lif

IP54 only 0.9kg 8+hours

• Curved surface correction

• DGS /AVG /DAC Curve

• RF Display Mode

• R-scan (1 hour )

• AWS D1.1 Evaluation

• Auto-calibration
• API 5UE evaluation

• 1000 Frames of A-scan Storage

► 640MHz sampling frequency , 800×480 full WVGA resolution assure quick and accurate display and analysis on defect signals .
► High signal-to-noise ratio, special composite materials, highly-attenuated or thick work-pieces.
► 4.3 inches display, set-in battery and charger, but only 0.9kg in weight
► Standard of IP54 certification and compatible with EN 12668:2000 standard.
► With full WVGA TFT display at industrial level, offers fine images at different angles.
► Auto-calibration function including fast calibrating material velocity, probe delay and probe angle.
► DAC: Easy to make, correct, store and recall DAC.
► USB port for software updating, data transferring and printing and access to devises such as mouse, keyboard and U-disk.

Transmitter Pulse | -Ve Square Wave Pulse,Transmitter Pulse Voltage:25～250V, continuously adjustable with 25V increments
Test Modes | Pulse echo and dual transmission
Damping | 400,80 Ohm
Frequency | Broadband/narrowband optional.Broadband:0.5～20MHz. Narrowband:1.5～3MHz
Gain | 0.0～110.0dB.Steps as 0.1/1.0/2.0/6.0dB
Material Velocity | 1000～15000m/s continuously adjustable.Set-in 30 common material velocities selectable
Test Range | 0.0～10000mm longitudinal wave at steel velocity. Range continuously variable with minimum 0.1mm increments
Rectification | Positive halfwave, negative halfwave, full wave, RF
Alarm | Real-time alarm signal, positive and negative thresholds, minimum depth, DAC alarm optional
Measuring Mode：Select front edge or peak of pulse wave in gate
Display | 4.3" industrial-leveled TFT color LCD with 800×480 WVGA resolution
Pulse Shift | -7.5～3000μs
Probe Zero | 0～999.9μs
Pulse Repetition Frequency | 25～800Hz, auto adjustment mode
Vertical Linearity Accuracy | ≤3%
Horizontal Linearity Accuracy | ≤0.2%
Surplus Sensitivity | ≥60dB(200Ф2 flat bottom hole)
Resolutions | ≥36dB(5P14)
Dynamic Range | ≥32dB
Reject | (0～90)%
Electric Noise Level | <10%
Interface | Q9 transducer cable connectors
USB HOST
Power Supply | Large-capacity lithium battery without memory effect; More than 8 hours
Built-in charger, AC Mains 220V
Dust/Splash /Water-proof | meets IP54 standard
Standards | EN12668-1 compliance
Conform to JB/T 10061-1999 standard
Environmental Temperature | -30～50℃
Relative Humidity | 20%～95%RH
Weight | 0.9Kg(with battery and built-in charger)
Dimension | TOP：215mm×126mm×53mm / bottom：215mm×104mm×42mm

Related Products

##### KFD-50 / 50X

##### KFD-30

- Previous

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.