###
Products

# KC-160

- Next

Description

-Auto recognition of the substrate material (Fe or NFe)
-Large and clear TFT Screen (1.8’ TFT 262K)
- Power supply:2 x1.5v AAA
- Auto power off

Technical Specification

| KC160
Operating principle | magnetic induction/eddy current (F/NF) Fe & NFe 2 in 1
Measuring Range | 0~1250μm, 0~49 mils
Resolution | 0.1 μm
Accuracy | ±((1-3)%H+2um)
Min.measuring area | 2*2 mm
Minimum curvature radius convex | 2mm
Minimum curvature radius concave | 25mm
Minimum thickness of substrate | 0.5mm
Battery indicator | low battery indicator
Metric/imperial | Power supply
Display | AVE,MAX,MIN,DEV
Measurement | Single
Operating temperature | 0～40℃
Power supply | 2 pcs. AAA Battery
Dimensions | 90×50×25mm
Weight | 41g

Related Products

##### KC-260F /260N /260FH

##### KC-300

- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.