###
Products

# KT-360

- Previous
- Next

Description

Display Resolution: mm 0.001 , 0.01 , 0.1; inch: - 0.001, 0.01

Large LCD backlight: 128 x 64 ( dot - matrix ) Hand held, small dimensions and light - weight

Operating Principle | Pulse echo with dual element transducers
Units | mm or inch
Measuring Range | 1.00～300.0mm(0.039～11.81inch)
Thickness Display Resolution | mm - 0.001, 0.01, 0.1; inch – 0.001, 0.01
Measurement Accuracy | 0.5%H+0.08mm(H – Thickness of the tested material)
Material Velocity Range | 1000 to 9999m/s
Measuring Range for Steel Pipes | Min. 20 diameter, 2.0mm thickness
Probe Zero Adjustment | 1 or 2 point calibration option included
V-path Correction | Automatic
Operating Mode | Normal mode, minimum capture mode, differential mode, HI / LO thickness limits
Pulse Repetition Frequency | 4Hz in normal measurement mode;16Hz in minimum capture mode
Display | Large LCD with backlight; 128×64 dot-matrix
Dialog Languages | English
Coupling Status Indicating | Coupling status symbol indicates whether satisfactory acoustic coupling between the transducer and test piece has been achieved
Battery | Two 5# AA alkaline batteries
Battery Life | 200 hours (with backlight off)
Low Battery Indicator | Continuously indicates battery status
Auto Shut-off | After 3 minutes of non-use
Data Logger | Up to 2000 readings
Interface | USB port allows communication with PC (OPTIONAL )
Dimensions / weight | 138mm×70mm×34mm / 230g with battery

Related Products

##### KT-400

##### KT-6 / KT-7 ( E-E )

##### KT-560

##### KT-500/500D/500DL

##### KT-300D / 310D

##### KT-300 / 310

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.