###
Products

# KH-220

- Previous
- Next

Description

Advantages

- OLED high lighting display

- USB communication interface with Data-view Software

- Automatic identification of any impact test direction

- Optional configuration support Bluetooth printing and wireless data transmission

- Directly use D / DC / D+15 / G / C / DL Impact device

- Memory of 600 average readings

- Upper and lower limit pre-setting

- Software calibration

Technical Specifications :

Measuring range : HLD(170~960)HLD

Measuring direction : 360°

Hardness Scale : HL,HB,HRB,HRC,HRA,HV,HS

Display : dot matrix LCD , 128×64 dots

Data memory : 600 groups max.(relative to impact times 32~1)

Printing paper : width is ( 57.5±0.5) mm, diameter is 30mm

Min. Radius of Workpiece : Rmin = 50mm (with special support ring Rmin= 10mm)

Min. Workpiece weight : 2~5kg on stable support

Min. Workpiece thickness : 3 mm (Impact Devices D/DC/DL/D+15)

Min. thickness of hardened surface : 0.8mm

Battery pack : 6V NI-MH

Battery charger : 9V/500mA

Continuous working period : about 50 hours ( 150 hours as optional battery )

Communication interface : USB1.1

Outline dimensions : 212mm×80mm×32mm

Related Products

##### KH-260plus

##### KH-320

##### KH-100S

##### KH-500

##### KUH-50

##### KH-180

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.