###
Products

# KGM3-F2

- Next

Description

Hand held Gloss meters

Type : KGM1-F2 ( 60 ° ，0.1 GU Resolution )

Description:

Memory, RS232, software. auto diagnosis, auto-calibrate

Technical Parameters | Unit | Parameter
Reading Range | GU | 0～ 1000
Deviation | GU | ±1.5; ±1.5%
Measuring Area | mm2 | 9×16
Incidence Angle | Deg. | 60
Volume (L×W×H) | mm3 | 155×48×75
Main Weight | g | 400
Power supply | One AA-size battery, 1.2v-1.5v,Rechangeable or alkaline

● Interface: Serial RS 232

● Software: Data Operator included.

● Memory: 10000 measurements or 999 data groups

● Power Supply: A single battery only. AA size, Rechargeable or alkaline

Related Products

##### KGM1-F1

##### KGM1-C1

##### KGM1-S1

##### KGM1-F2

- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.