###
Products

# KUP-300

Description

Ultrasonic PD measurement tool

TEV measurement :

Sensors: Capacitive

Measurement Range ：-5~ 60dB ，step length 1dB .

Resolution ： 1dB

Accuracy ： ±1dB

Max Number of Pulses/Cycle ； 655

Ultrasonic measurement :

KUP-300Measurement Range : -11dB ~ 68dB , step length 1 dB

Resolution : 1dB

Accuracy : ±1dB

Transducer Sensitivity : -65dB（0dB = 1volt/µbar rms SPL）

Transducer Centre Frequency : 40kHz

Transducer Diameter : 16mm

Heterodyning Frequency : 38.4kHz

Weight : 1kg (host) 0.5kg (sensors) Size: Host 245 * 132 * 45 mm

Power Supplies

Rated Voltage : 90 ~ 264 V

Frequency : 47~ 63 Hz

Typical Operating Time : approx. 5 hours

Internal Batteries : Lithium-ion

Features

● Ultrasound, TEV PD waveform and three-section indicative values (yellow, green, red ) are in the same interface

● Take dBmV as the unit and use Transient Earth Voltage （TEV）to detect the size of partial discharge.

● Use colored LCD (Liquid Crystal Display), the display effect is more intuitive and more friendly

Related Products

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.