###
Products

# KT-6 / KT-7 ( E-E )

- Next

Description

Features:

●Metric-inch free convertible. Display : 0.01mm/0.001inch

●Two modes for through coating measurement: normal test model T-E ,Through coating model E-E ,without removing the coating with KT7

●USB data interface communication, transferring with PC and outputting data with “.txt.”

●Large data storage capacity, Max. Up to 2000 groups. Every group can reach to 99 data.

●7 practical measurement modes available: Standard Mode, Scanning Mode, Difference Mode, Average Mode, Maximum Limitation Alert Mode, High Temperature Mode(should be matched with high temperature probe)

●Probe Zero function, Sound Velocity Calibration function

●Button keyboard designing for convenient shortcut operations for Probe-zero function, One-point and Two-point calibration, as well as numerical adjusting with direction key control.

Product Specification:

Model | KT6 | KT7
Measurement Range | 0.65~400mm
Measuring Range(Through Coating) | / | 3~20mm
Material Velocity Range | 509~18699m/s
Measuring Accuracy | ±(0.5%H+0.05)mm
Display Accuracy | 0.01mm/0.001inch
Scanning Rate | 2~20 times/sec
Frequency Bandwidths | 1～10MHz
Measuring lower limit of pipes | Φ15mm×1.0mm (Probe: 5MHz, Φ10mm) Φ10mm×1.2mm (Probe: 7.5MHz, Φ6mm)
Display Mode | 128×64 matrix LED
Power supply | 2 AA Alkaline Batteries
Operating Time | 280 hours typical battery life, 100 hours continuous with backlight on
Operating Temperature Range | -10℃～50℃(Ambient Environment) -10℃～300℃(High Temperature Mode)
USB | √
Gauge Size | 136 mm×72 mm×20mm
Weight | 176g（Including Batteries）

Related Products

##### KT-360

##### KT-400

##### KT-560

##### KT-500/500D/500DL

##### KT-300D / 310D

##### KT-300 / 310

- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.