###
Products

# AT3 / AT7

- Previous
- Next

Description

Hand held thermal imaging camera

Specification

Items | AT3 | AT7
Detector characteristics | Detector type | Un-cooled FPA micro-bolometer
Array size/format | 160×120 | 384x288
Image characteristics | Field of view/Min focus distance | 25°×19°/0.1m
Spatial resolution（IFOV） | 2.73mrad
Thermal sensitivity | ≤0.08℃@30℃ | ≤0.06℃@30℃
Frame frequency | 50Hz
Focus | Manual
E- Zoom | x 2
Spectral range | 8-14um
Built-in CCD camera | 1.3 million pixels, COMS camera modules
Image display | LCD display | 2.7”TFTLCD，320×240
Measurement | Temperature ranges | -20℃- +350℃ | -20℃- +600℃
Accuracy | ± 2°C or ± 2% of reading, Whichever is greater
Measurement correction | Automatic / manual
Measurement mode | Up to 4 movable spots. Up to 3 movable areas. Up to 2 movable lines (maximum, minimum and average temperatures). Line profile. Isotherms. Temperature difference. Alarm (voice, color)
Image control | Color palette | 11palettes changeable
Image adjustment | Auto/manual gain and brightness
Setup functions | Date/time, temperature unit ℃/℉/K, language
Emissivity correction | Variable from 0.01 to 1.0,or correct it according to predefined form
Background temperature correction | Automatic
Atmospheric transmission correction | Automatic correction according to user input object distance, humidity and temperature
Image storage | Storage card | 2G SD card, max 16G
Storage mode | Manual/Auto single file saving, IR and Visual image link saving
Thermal image format | JPEG with original thermal measurement data included
Visual image format | JPEG
Voice annotation | Input via built-in microphone up to 60 seconds of digital voice clip per image stored with image
Laser pointer | Laser locator | Class 2, 1mw/635nm(red)
Power source | Battery type | Li-Ion, rechargeable
Battery operating time | 3 hours continuous operation
Battery charging mode | Intelligent charger or power adaptor 12V(optional) charge
Power saving | Auto-sleep and auto-shut down
External power | 12V DC
Environment | Operating temperature | -15℃-+50℃
Humidity | ≦90％（non-condensing）
Encapsulation | IP54
Drop test | 2m
Physical characteristics | Weight | 1Kg
Dimension | 105mm×245mm×230mm
Interface | SD card slot | Micro SD
External DC input | yes
Video output | yes
Data output | USB

Related Products

##### AT4 & AT8

##### AT15 & AT35

##### AT60S

##### ATB6

##### ATH1

##### AT1B

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.