###
Products

# KT-400

- Previous
- Next

Description

Color 320x240 Pixels Display A-Scan Snapshot

Echo-Echo Mode(Thru Paint & Coatings) Stores 100,000 Readings

Gain: Low, Medium or High for varying test conditions

KT-400 Series Technical Specifications

Feature | KT-400 | KT-400D | KT-400DL | Data Logger Option
Color Display | ü | ü | ü |
A-Scan Snapshot | ü | ü | ü |
Gain: Low, Medium, High | ü | ü | ü |
Min/Max Capture | ü | ü | ü |
DIFF/RR% | ü | ü | ü |
Thru-paint | X | ü | ü |
Data Logger | Optional | X | ü | ü
DataView Software | Optional | X | ü | ü

Instrument Specifications
Display Type | 2.4" color OLED, 320 X 240 pixels, contrast 10,000:1
Operating Principle | Pulse echo with dual element transducers
Measuring Range | 0.60mm to 508mm(0.025" to 20.00"), depending on material, probe and surface condition
Measuring Resolution | Selectable 0.01mm, 0.1mm(selectable 0.001", 0.01")
Units | Inch or Millimeter
Gain | Low, Medium or High for varying test conditions
Display Mode | Normal, Minimum / Maximum capture, DIFF/RR%
V-Path Correction | Automatic
Update Rate | Selectable 4Hz, 8Hz, 16Hz
Material Velocity Range | 500 to 9999m/s (0.0197 to 0.3937in/us)
Languages | Selectable Chinese, English, Japanese
Alarm Settings | Minimum and Maximum alarms. Range of 0.25 mm to 508 mm (0.010" to 20.00"). Dynamic waveform color change on alarm
Power Requirements | 2 AA size batteries
Operating Time | Approximately 40 hours
Instrument Shut-off | Selectable ALWAYS ON or AUTO OFF after 5, 10, 20 minutes of inactivity
Operating Temperature | -10°C to +50°C (+10°F to +120°F)
Size | 153mm X 76mm X 37mm(H X W X D)
Weight | 280g including batteries

Data Logger Option Features
Capacity | 400 files, 100,000 readings
File Structure | Grid file
Rows X Columns | 21 X 12
Communication Port | USB 2.0 (Full Speed ) port
Software | DataView PC software

KT-400 Probe/Transducer Specifications
Model | PT08 | TC510 | PT12 | ZT12 | PT06 | PT04 | GT12
Type | KT-400 Standard | KT-400D/DL Standard | Optional Standard | Cast iron | Small tube | Fingertip | High-Temperature
Frequency | 5MHz | 5MHz | 5MHz | 2MHz | 7.5MHz | 10MHz | 5MHz
Contact Diameter | 11mm | 13.5mm | 13.5mm | 17mm | 8mm | 6mm | 15mm
Measurement Range | 0.8 to 100.0mm | General 1.0 to 200.0mm Through Mode 2.5-25mm | 1.0 to 200.0mm | 4.0 to 508.0mm | 0.8 to 30.0mm | 0.7 to 12.0mm | 4.0 to 80.0mm
Temperature Range | -10 to 70℃ | -10 to 70℃ | -10 to 70℃ | -10 to 70℃ | -10 to 70℃ | -10 to 70℃ | -20 to 300℃

Related Products

##### KT-360

##### KT-6 / KT-7 ( E-E )

##### KT-560

##### KT-500/500D/500DL

##### KT-300D / 310D

##### KT-300 / 310

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.