###
Products

# KFD-30

- Next

Description

Mini Ultrasonic Flaw Detector KFD-30 is a hand-held model, both Flaw Detector and Thickness Gauge 2 in 1, Light weight. It provides users most of features of large models. Here please check the features below:

High resolution TFT color screen

● Auto zero calibration
● DAC and AWS curve
● Welding simulation map display, filled waveform trace display
● Freeze and peak memory mode
● Separately Gate A and Gate B setting with alarm
● Echo-echo for thru coating thickness measurement
● Peak or Flank measurement
● T-scan
● Display sound path value, surface distance and depth to flaw in angle beam ● inspections
● Large memory of 500 test report with A graph in flash memory
● Li battery, continuously work up to 9 hours
● Data transfer and print thru USB

# Standard Delivery:

Main unit
Straight transducer
Angle transducer
Transducer cable
Hand-held belt and shoulder strap
Battery pack
AC adapter/Charger
Software
USB cable
Calibration certificate
Instruction manual
Carrying case

# Technical Specification:

Measuring Range | 0.0-6000.0mm
Sound Velocity | 3240m/s and 5920m/s are stored or input the new velocity from 1000-9999m/s
Gain | 0-100dB, adjustable in step of 1/2/6/12
Frequency Range | 0.5-15MHz
Probe delay | 0-365μs
Test methods | Pulse echo mode (T-E) and Thru mode (E-E)
Pulse Voltage | 300V negative spike
Damping | 100Ω
Echo Presentation | Full wave
Unit | Mm or inch
Horizontal Linearity Error | ＜0.1%
Vertical Linearity Error | ＜3.0%
Resolving power | ＞32db
Sensitivity Leavings | ＞58db
Dynamic range | ＞32db
Gate | Height adjustment of zoom in and out
DAC curve | Choice at any point
Print Output | Waveform and data storage
Display | 3.5” true color display 320╳240
Battery working time | 9 hours
Operating Temperature | -20℃-+50℃
Power Supply | 4.2VDC, 220VAC
Dimensions & Weight | 122╳82╳23.8mm, 430g including battery

Related Products

##### KFD-50 / 50X

##### KFD-55

- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.