###
Products

# KR-100

- Next

Description

Features:

Pocket-size & economically price;
Useing the high speed microprocessor DSP;
Using the OLED screen,bright and without visual angle
Data ourput USB port
Large measuring range suitable for most materials
Measures flat,outer cylinder and sloping surface
Both Ra and Rz parameters in one insrument
Works on 3.7V rechargeable lithium-battery,work while charging
Real time battery indicator
Technical Specifications:

Roughness parameter | Ra,Rz,Rq,Rt
Tracing length | 6mm
Tracing speed | 1.0mm/sec
Cut-off lengths | 0.25mm/0.8mm/2.5mm
Evaluation length | 1.25mm/4.0mm
Measuring range | Ra,Rq: 0.05-10.0μm Rz,Rt: 0.1-50μm
Accuracy | ±15%
Repeatability | <12%
Radius and angle of the stylus point | Diamond,Radius : 10μm±1μm Angle: 90°(+5°or -10°)
Power supply | 3.7V Li-ion battery
Recharging time | 3 hours
Operating temperature | -20-40 ℃
Relative humidity | <90%
Dimensions (L×W×H) | 106×70×24mm
Weight | 200g
Standard Deliver
Main Unit KR-100 | Specimen Ra
Charger | USB Cable
Instruction manual | Suitcase

Related Products

##### KR-230

- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.