###
Products

# KT-300D / 310D

- Previous
- Next

Description

FEATURES:

AUTOMATIC SELF CALIBRATION

COUPLANT INDICATOR

AUTOMATIC POWER OFF DEVICE

HIGH-LOW LIMIT ALARM

LCD BRIGHTNESS ADJUST

THROUGH COATING CAPABILTY

LOW BATTERY INDICTOR

TECHNICAL SPECIFICATIONS :

| KT-300D | KT-310D
MEASURING RANGE (STEEL) | STANDARD | 0.8mm – 250mm Depending of the probes
THROUGH COATING | 3mm – 18mm Depnding of the probes
DISPLAY RESOLUTION | 0.1mm or 0.01inch | 0.1mm/0.01mm or 0.01inch/0.001inch
TOLERANCE | +/- 0.1mm in steel | +/- 0.025mm in steel
VELOCITY RANGE | 1000-9999 m/s (0.0393-0.3936 inch/μ s)
DISPLAY TYPE | 4 digital LCD with advanced backlight
MEMORY | 500 Test Values
POWER | 2 pcs. 1.5v AA Batteries
OUTSIDE DIMENSION | 149mm×73mm×32mm
WEIGHT | 160g

STANDARD DELIVERY :

1.MAIN UNIT WITH THROUGH COATING MODE

2.STANDARD PROBE PT-08

3.COUPLANT BOTTLE

4.TWO AA SIZE 1.5V BATTERIES

5.OPERATION MANUAL

6.CARRYING CASE

Related Products

##### KT-500/500D/500DL

##### KT-560

##### KT-6 / KT-7 ( E-E )

##### KT-300 / 310

##### KT-100B/200B

##### KT-100D/200D

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.