###
Products

# KT-300 / 310

- Previous
- Next

Description

Features:
AUTOMATIC SELF CALIBRATION

COUPLANT INDICATOR

AUTOMATIC POWER OFF DEVICE

HIGH-LOW LIMIT ALARM

LCD BRIGHTNESS ADJUST

LOW BATTERY INDICTOR
Technical Specifications:

| KT-300 | KT-310
Display Resolution | 0.1mm (or 0.01 inch) | 0.1mm/0.01mm or 0.01 inch /0.001inch
Accuracy | ±(1%H +0.1)mm | ±(0.5%H + 0.01)mm
Measuring Range | 0.8 - 300.0 mm depending on the probes (1.0 - 200.0 mm with Standard Probe within the package)
Display Frequency | 4Hz
Memory | Store up to 500 test values
Sound velocity | 1000-9999 m/s (0.0393-0.3936 inch/μ s)
Display Type | 4 digital LCD with advanced backlight
Power Supply | 2 pcs. 1.5v AA standard Batteries
Working temperature | -0 ºC ~ +50 ºC
Dimension | 149 mm X 73 mm X 32 mm
Weight | 168g (main unit); 30g (standard probe)

Features:
AUTOMATIC SELF CALIBRATION

COUPLANT INDICATOR

AUTOMATIC POWER OFF DEVICE

HIGH-LOW LIMIT ALARM

LCD BRIGHTNESS ADJUST

LOW BATTERY INDICTOR
Technical Specific Features:

AUTOMATIC SELF CALIBRATION

COUPLANT INDICATOR

AUTOMATIC POWER OFF DEVICE

HIGH-LOW LIMIT ALARM

LCD BRIGHTNESS ADJUST

LOW BATTERY INDICTOR
Technical Specifications:

Probes | Frequency | Diameter | Measuring Range (steel) | Application
PT-12 | 5 MHz | 12mm | 1.0-200mm | Standard Probe
PT-08 | 5 MHz | 10mm | 0.8-100mm | Standard Probe
PT-06 | 7.5 MHz | 7.6mm | 0.8-30.0mm | Miniature Probe
ZT-12 | 2 MHz | 16.2mm | 4.0-300mm | Lowe frequency Probe
PT-04 | 10 MHz | 5mm | 0.8-20.0mm | Minisize Probe
GT-13 | 5 MHz | 14mm | 4.0-80.0mm | High Temperature probe

Related Products

##### KT-300D / 310D

##### KT-500/500D/500DL

##### KT-560

##### KT-100B/200B

##### KT-100D/200D

##### KT-350

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.