###
Products

# AT15 & AT35

- Previous
- Next

Description

Hand held Thermal imaging camera

Technical Specifications

Item | AT15 | AT35
Detector Data |
Detector Type | Uncooled FPA,160×120 pixels | Uncooled FPA, 384×288 pixels
Pixel pitch | 25μm
Spectral range | 8~14μm
IFOV/Mini Focus | 21°×16°/0.15m (standard lens) | 21°×16°/0.4m (standard lens)
42°×32°/0.1m (wide lens,optional) | 38°×28°/0.3m (wide lens,optional)
10°×8°/1m (telephoto lens,optional) | 11°×8.5°/1.2m(telephoto lens,optional)
Spatial resolution(IFOV) | 25μm
Spectral range | 8~14μm
IFOV/Mini Focus | 21°×16°/0.15m (standard lens) | 21°×16°/0.4m (standard lens)
42°×32°/0.1m (wide lens,optional) | 38°×28°/0.3m (wide lens,optional)
10°×8°/1m (telephoto lens,optional) | 11°×8.5°/1.2m(telephoto lens,optional)
Spatial resolution(IFOV) | 2.3mrad | 1.2mrad
Sensitivity/NETD | <60mk @ +30 | <80mk @ +30
Image Presentation |
Image Display | 3.2” 270° tiltable LCD
Image modes | Thermal image, visual image, thermal fusion,picture-in-picture, thumbnail gallery
Thermal fusion | IR image shown above, below or within temp interval on visual image
Picture in Picture | Resizable and movable IR area on visual image
Frequency | 50Hz(PAL)/60Hz(NTSC)
Focus | Auto/Motor
Digital Zoom | 1-4x Continous | 1-8x Continous
Visual camera | 3.0 mega pixel
Spotlight | 10cd/m²
Measurement |
Temperature range | -20 ~ 250 (Industrial)
-20 ~ 600 (optional A)
-20 ~ 1200 (optional B)
Temperature Measurement accuracy | ±2 or ±2% of reading
Spotmeter | 4 adjustable spots
Area | 3 adjustable boxes with max./min./average
Line profile | Horizontal/vertical
Isotherms analysis | Detect high/low temperature/interval
Dew point alarm | No
Hot/cold spot Auto detection | Max/Min/Average temp
Emissivity correction | Variable from 0.01~1.0
Alarm | Voice and Color
Multiple language menu | 10 languages (English,French,Italian,German,Spanish,Portuguese, Russian, Korean, Japanese, Chinese)
Set-up Commands |
Real-time Video | Transfer via USB
Color palettes | Iron, anti-iron,feather red,black hot,white hot, medical
Set-up commands | Date/time, temperature units C/F/K, language, scale
Measuring Calibration | Automatic, based on inputs
Image Storage |
Storage type | 4G SD card, Building-in flash
Storage capacity | Up to 700 images in built-in flash card | Up to 500 images in built-in flash card
Up to 11200 images in 4G SD card | Up to 8000 images in 4G SD card
Storage format | Standard JPEG, including measurement data
Periodic image storage | user definited, 7 seconds at least
Laser Pointer |
Grade/Type | Class II, 1mW/635nm red
Power System |
Battery | Li-ion, ≥3 hours operating time
Charging system | In camera or AC adapter
AC supply | 110 240V AC 50/60Hz 5V DC output
Voltage | 5V±5% DC
Power management | Automatic shutdown(user selectable)
Environmental Data |
Operating temperature range | -20+50
Storage temperature range | -40+70
Humidity | ≤90% non-condensation
IP level | IP54
Physical Data |
Weight , size ( LxWxH) | 390g , 128×62×154mm
Data Communication Interfaces |
USB | Data transfer to and from PC
Video output | PAL/NTSC
Audio output | Yes
Packing |
Standard | Thermal imaging camera with Standard lens, 2 Batteries, Battery charger, USB cable, SD card, SD card reader, CD-ROM software and user manual), Adapter, Warranty card, Calibration certificate
Optional Accessories | Infrared lens, Li-ion battery

Related Products

##### AT60S

##### ATB6

##### ATH1

##### AT4 & AT8

##### AT3 / AT7

##### AT1B

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.