###
Products

# KV-170P

- Previous

Description

Features:

●Multi-parameter vibration, bearing parameter & IR temperature measuring

●One button control power, parameter selection, measurement and holding.

●With remote switch and magnet base to avoid handheld problem to get reliable and consistent data.

●Measuring vibration velocity, displacement & acceleration envelope to check machine/bearing health ►with yellow/red/green LED indicator

●Build-in International standard (Mechanical Vibration )

●With magnet base and remote switch

●Sensor included, Easy to use.

●Automatic power off. 4 digital LCD display

●Metal case, Robust, Reliable

●Both Metric & English Unit selectable

Specifications:

Accuracy : ± 5% ± 2 digits

Measurement Range & Frequency response:

Acceleration: 0.1 to 100 m/s2 / 0.01 to 10 g / 10Hz~3kHz peak

Velocity:0.1 to 250 mm/s / 0.01 to 15 inch/s / 10Hz~1000Hz RMS

Displacement: 1 to 3000 µm / 0.03 to 120 mil / 10 Hz~500Hz peak-peak

Enveloped Acceleration: 0.1 to 25 unit / 5Hz~2kHz demodulated from 3kHz~10kHz

Temperature: -33 to 220 oC / -27.4 to 428 oF

Battery: 1/2 AA, 3.6V, 20-29mA, >100 hours of continuous operation.

Pickup: Integrated accelerometer with extension stinger and magnet base

Dimensions: 110x35x17 mm; Weight: 100 g (Including battery)

Related Products

##### KV-130

- Previous

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.