###
Products

# KT-100D/200D

- Previous
- Next

Description

Features
The Through-Coating thickness measurement (E-E)

Pocket Size, easy to operate

Automatic Probe Zero calibration

Automatic probe identification

Measuring Range: E-E: 4-25mm

T-E: 0.65-400mm

(Range depends on probe-material combination)

Memory: 5000 readings with location number (KT-200D)

Data output: USB to PC (KT-200D)

Three measurement modes: T-E, E-E, Scan 9 material velocities are stored for selection,Or input the new velocity manual

Technical Specification

Specification | KT-100D | KT-200D
Measurement mode | Transmit-echo | -Standard measurement: For Normal thickness measurement. -Minimum measurement: For curved surface -Differential measurement: Displays the difference from the actual thickness -measurement and a user entered reference value Average measurement: 2-9 point selectable -Limit measurement: Min. Max setting and alarm | √ | √
Echo-Echo | The metal wall thickness is accurately and quickly measured in spite of surface coating | √ | √
Scan | Thickness value at 10 measurements per second while also display actual thickness (Ideal for high temp. thickness readings) | √ | √
Probe identify | Auto | √ | √
Probe zero | Auto at power up and continuously during the measurement | √ | √
Gain adjust | Auto gain adjustment Manual gain adjustment, low, standard and high | √ | √

Related Products

##### KT-100B/200B

##### KT-300 / 310

##### KT-300D / 310D

##### KT-500/500D/500DL

##### KT-560

##### KT-350

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.