###
Products

# KGM1-C1

- Previous

Description

Hand held Gloss meters

Type: KGM1-C1 ( 60 °, 0.1 GU Resolution )

Description: Small, stable, precise. AA-size battery.
Standard: ISO2813, ISO7668, ASTM D523, ASTM D 2457, GB/T 9754, GB/T 13891, GB/T 7706

Measuring Angle | 60°
Detecting range | 0~199.9Gu
Stability | within ±0.4Gu/30Min
error limit | within ±1.0Gs
Power supply | 2 x 1.5V AAA
Light Spot size | 10×20mm
Measuring hole size | 20×40mm
Temperature | 0-40°C Relative
Relative humidity | below 85%
Dimension of instrument | 112mm×32mm×68 mm
Weight of instrument | 200g

Related Products

##### KGM1-S1

##### KGM1-F1

##### KGM1-F2

##### KGM3-F2

- Previous

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.