###
Products

# ATH1

- Previous
- Next

Description

●Architectural Problems

●Electronic industry ,mechanical inspection

●Researching system

●Automation application system

Features :

●Compact in size of only 125*72*16mm, small volume

●Quick start , measuring at any time .

●Central point temperature measuring and automatic tracking of highest / lowest temperature points.

●3.5-Inch large screen , auto rotation

●50-degree field of view for instant finding.

●USB 3.0 Type-C port for data transfer and recharging.

●Three-key operation mode for easy use even by green hand.

Item | Specification
Overview | Size of Screen | 3.5 inch
Resolution of Screen | 480 * 320
Images Stored | 600
Image Format | BMP
Data/Recharging Port | USB3.0 Type-C
IR Temperature Measurement | Resolution of Sensor | 80 * 60
Measurement Precision | ±2℃ ~ ±2%
Measurement Range | -20 ~150℃
Radiation Ratio | 0 ~ 0.95 adjustable
D:S | 15:1
Thermal Sensitivity | <50mK @ f/1.0
Wavelength Range | 8 μm to 14μm
Temperature Measurement Function | Central point temperature measuring, automatic tracking of highest/lowest temperature points.
IR Image | Frame Frequency | 9Hz
Angel of View | 50° * 38.6°
Palette | Iron red, rainbow, gray
Protection | Protection Grade | IP54
Miscellaneous | Battery Type | Rechargeable lithium battery
Consecutive Operation Duration | ＞4 hours
Dimensions | 125 * 72 * 16mm
N.W | 170g
G.W | 420g
Package Include | Power Adapter, USB Cable, Wrist Strap, Quick Start Guide, Certificate Card, Warranty Card
Other Sensor | Direction sensor
Operating Temperature | 0℃ ~ 45℃
Storage Temperature | ﹣20℃ ~ 55℃

Related Products

##### AT5X

##### AT3B

##### ATB8

##### ATB6

##### AT60S

##### AT15 & AT35

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.