###
Products

# KV-130

- Next

Description

Features:

1.Solid Metal Shell

2.Extremely reliable and potable, low cost instrument

specifically designed for on site maintenance in

your plant or workshop. It measures overall

vibration level by velocity RMS. Displacement

Peak_Peak & Acceleration Peak.

3.With one-button operation, holding function and

automatic power off.

4.With one-button operation, holding function and

automatic power off.

Specifications:

Measurement Range | Velocity RMS (mm/s) 0.2 ~199.9mm/s Displacement Peak_Peak 1~1999 micron Acceleration Peak 0.2 ~180 m/s
Accuracy | 5 2 digits
Frequency response | Acceleration Peak:10~1000Hz(0.5dB 2 digits),1000～4000Hz(3dB2 digits) Velocity RMS: 10Hz < f < 1000Hz, 10% Displacement Peak_Peak: 10Hz～1000Hz (0.5dB 2 digits)
Display | 4 digits LCD, refresh interval about 0.5 second
Power supply | 1/2 AA, 3.6V, Operation Current 4-7mA
Battery capacity | >100 hours continuously or 4000 times measurement
Operation environment | Operation Temperature: 0 C~50 C;
Dimension: | Relative humidity: < 85% (WxDxH)
Weight | 160mm x 25mm x 17mm 120g (include batteries)
Case Material | Aluminum

Standard delivery:

Vibration meter

Long needle

Magnet base

Remove Control

Small pocket bag

User’s Manual

Battery (Inside meter)

Certificate

Related Products

##### KV-170P

- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.