###
Products

# KBT-10SA

- Previous

Description

Accurately, quickly, reliably, movably to measure Brinell indention

Using CCD camera to capture the indention image, instead of reading diameter from microscope by operator then calculating.

As an independent measurement system, Matching any kinds of Brinell hardness tester

Special software supplying simplest operation

Both single testing and batch testing mode are available

Tolerance setting ,distinguishing and alarming

Statistics values such as Max, Min, Avg, R and S are available

Convert test result to other scales, such as HRC,HRB,HRA,HV,σb

All test data and indention images are saved automatically

Test report created in Microsoft EXCEL format, can be edit, copy, print as you will

Measuring scope from 7.96HBW to 658HBW

Software update freely

SINGLE TEST BATCH TEST

SCALE CONVERSION TOLERANCE SETTING

Standard delivery：

Cables 2

CCD camera 1 Soft dog 1

Power & USB module 1 Shockproof suitcase 1

Software disc 1

Version : win7,WIN xp / win10

Related Products

##### KH-160

##### KUH-50

##### KH-500

##### KH-100S

##### KH-320

##### KH-260plus

- Previous

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.