###
Products

# KC-260F /260N /260FH

- Previous
- Next

Description

KC-260 Series

Coating Thickness Gauge

Measuring principle
Magnetic Method (Fe): Measuring the thickness of non- magnetic coatings on steel, iron and other ferromagnetic metal substrates, e.g. painting, varieties of anti-corrosion coating, powder spraying, plastic, rubber, synthetic material, phosphate coating, chromium, zinc, Aluminum, tin and cadmium, etc.
Eddy Current Method (NFe): measuring the thickness of non-conductive coatings on copper, aluminum, stainless steel and other non-ferromagnetic substrates, e.g. painting, varieties of anti-corrosion coating, powder spraying, plastic, rubber, synthetic material, oxide film and phosphate film, etc.
Specification

Model | KC-260F | KC-260N | KC-260FH
Measuring Principle | Magnetic Method | Eddy Current Method | Magnetic Method
Measuring Range(μm) | 0-3000 | 0-2000 | 0-10000
Display Resolution (μm) | 0.1 reading | 0.1 reading | 10
Repeatability | ±(1%H+1) | ±(1.5%H+10)
Accuracy (μm) | ±(2%H+2) | ±(2%H+10)
Testing Condition(mm) | Min. Curvature Radius(凸) | 1.5 | 3 | 10
Min. Measuring Surface | ∮7 | ∮5 | ∮40
Min. Substrate Thickness | 0.5 | 0.3 | 2

Standard Delivery

KC-260 Main Body with F1 or N1 or P3 probe | Calibration Foil set | Software & Communication USB Cable
Instruction Manual | Carrying Case |

Related Products

##### KC-300

##### KC-160

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.