###
Products

# KR-230

- Previous

Description

Features:

Electromechanical integration design, small volume, light weight, easy to use,

Using DSP chip to control and data processing, high speed, low power consumption,

20 parameters Ra, Rz, Rq, Rt, Rp, Rv, R3z, R3y, Rz(JIS), Rs, Rsk, Rku, Rsm, Rmr; Ry(JIS)=Rz; Rmax=Rt, RPc, Rk, Rpk, Rvk, Mr1, Mr2

128 x 64 OLED dot matrix display, digital / graphic display; highlight no perspective,

Display information rich, intuitive, can display all the parameters and graphics,

Compatible with ISO, DIN, ANSI, JIS national standards,

Built-in lithium ion rechargeable battery and a charging control circuit, high capacity, no memory effect,

Residual quantity indicator icon, prompting the user to charge,

Display of the charging process instructions, the operator can understand the degree of charge,

Working time more than 20 hours of continuous work,

Large capacity data memory, can store 100 groups of original data and waveform,

Real-time clock settings and display, convenient data recording and storage,

With automatic dormancy, automatic shutdown and power saving function,

Reliable control motor to go dead circuit and software design,

Measurement information display, menu prompt information, false information and switch machine and other tips that information,

Full metal shell design, sturdy, compact, portable, high reliability,

Can be in English freely switch,

Can be connected to a computer and optional Bluetooth printer,

Optional sensor surface, hole sensor, measuring platform, sensor, an extension rod and other accessories.

Technical Specification:

Roughness Parameters | Ra, Rz, Rq, Rt, Rp, Rv, R3z, R3y, Rz(JIS), Rs, Rsk, Rku, Rsm, Rmr; Ry(JIS)=Rz; Rmax=Rt, RPc, Rk, Rpk, Rvk, Mr1, Mr2
Standard | ISO,ANSI,DIN,JIS
Assessed Profiles | Roughness profile, Material ratio profile, direct Profile
Measuring Range | Ra 0.005μm ~ 16μm, Rz 0.02μm ~ 160μm
The maximum driving trip | 17.5mm/0.7inch
Resolution （Horizontal） | 0.01µm/±20µm, 0.02µm/±40µm, 0.04µm/±80µm,
Filter | RC, PC-RC, Gauss, D-P
Sample length (lr) | 0.25mm, 0.8mm, 2.5mm
Internal storage capacity | 100 groups of original data
Evaluation length(ln) | Ln=lr x n n=1-5
Pick up | Inductive, Diamond stylus with Radius 5 µm and angle 90°
Tolerance | ≤±10%
Repeatability | ≤6%
Output | USB
Power | Li-ion Battery rechargeable
Dimensions | 143 x 55 x 42mm
Weight | 400g

Standard delivery:

Main unit

Sensor

Adjustable Support

Calibration Block

Charger and USB cable

Carrying case

Operation manual

Calibration certificate

Related Products

##### KR-100

- Previous

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.