###
Products

# KT-100B/200B

- Previous
- Next

Description

Features
Pocket size, easy to operate
Automatic Probe Zero Calibration
Automatic Probe identification
Suitable for various materials such as steel, stainless steel, aluminum, glass,polystyrene, polyethylene
Average calculation of max 9 readings
Limits setting Low-High
Standard 5.0MHz transducer included, optional transducers 7.5MHz, 2.0MHz, 5.0MHz high temperature
Sound velocity range 1000 up to 9999m/s
Display resolution selectable at 0.1mm/0.01 inches and 0.01mm/0.001 inches
Memory of eadings with location number

Technical Specification

| KT-100B | KT-200B
Display: 128×64 with backlight | √ | √
Measuring range : 0.65-400mm (0.025-15.78inch) (range depends on probe-material combination) | √ | √
Velocity rate : 1000-9999m/s (0.0393-0.3936inch/us) | √ | √
Average mode: 2 to 9 times average measurement |  | √
Limit setting: With Low-High indication and alarm |  | √
Calibration : Auto | √ | √
Display Resolution: 0.01mm(0.001inch) for thickness up to 99.99mm (3.936 inch) 0.1mm(0.01inch) for thickness above 99.99mm (3.93 inch) | √ | √
Measuring units: mm/inch | √ | √
Memory: Memory of max. 5000 readings with location number |  | √
Data output: USB to PC |  | √
Surface temperature: -15℃ to +150℃ (special probes available) | √ | √
Battery indicator : Low battery voltage indicator | √ | √
Power supply : AAA dry cell 1.5V (2 pcs) | √ | √
Dimensions: 115 × 64 × 27mm | √ | √
Weight: 220g including batteries | √ | √

Related Products

##### KT-300 / 310

##### KT-300D / 310D

##### KT-500/500D/500DL

##### KT-560

##### KT-100D/200D

##### KT-350

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.