###
Products

# KC-300

- Previous

Description

*Various probes optional, probe auto matching.

* Two measuring modes are available: continuing measuring mode（CONTINUE）and single measuring mode（SINGLE）

* 2 methods can be used to calibrate the gauge ( zero calibration, two-point calibration ) ,and the system error of the probe can be corrected by use of basic calibrating method .

*Durable ruby probe, more wear and precise.

*Full metal shell design, sturdy, portable, high reliability.

*Alarm function when overrun the settable limiting range.

*Five statistics values [MEAN, MAX, MIN, NO., S.DEV] for higher accuracy.

*Large storage, easy to delete single or multiple saved values..

*PC software optional, convenient the data transmission, analysis, printing etc.

Measuring range | 0-1250μm, depends on probes, MAX 10mm for the probe F10.
Working principle | Magnetic & Eddy
Substrate | FE / NFE base
Resolution | 0.1μm
Display | 128x64 LCD with backlight
Accuracy | ±2%H+1um Note: H is thickness reading
Memory | 5 files x 100 values
Unit switch | Metric (μm) Imperial (mil)
Working temperature | Operation Temp. : -10~50°C Storage Temp. :-30~70°C
Power | AA battery 2pcs
Weight / Size | 340g / 115*67*31mm

Related Products

##### KC-260F /260N /260FH

##### KC-160

- Previous

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.