###

- Previous
- Next

# Metal Magnesium, Metal Calcium (with Latest Tech)

Description
Vertical Reduction Furnace, Metal Magnesium Plant, Metal Calcium Plant
The highly effective vertical metal magnesium reduction furnace /metal Calcium plant invented by is the international top technology and patent, the Only operation stability currently in domestic market, and the biggest productivity working in practical production, which can reduce 1/3 energy consumption, 15~30% comprehensive cost, contributing to national energy and environment, also strongly increasing the market competitiveness. We have contracted three of the domestic Top Five magnesium companies, two companies started to use vertical reduction tank from 2012, and reached the product quality and productivity within three months. As far, the domestic total of 92000 tons of metal magnesium products is from our high efficient vertical reduction tank technology.We are the China Pigeon Mg plant.
Metal Magnesium industry metal Calcium plant is a labor-intensive enterprise, and the main section to determine the labor amount is the feeding and slag-removal for the reduction furnace. The reduction furnaces select two sets of 128tanks Vertical reduction furnace, its advantages compared with horizontal tank reduction furnace are as bellows:
1. The reduction furnaces are only two, low area cover, less civil investment.
2. The low labour number, reduction furnace operator is less than 70 for 10000ton Mg, reducing half than horizontal furnace.
3. Single tank are larger productivity, three times than horizontal tank, but longer reduction time, 14~16hours, it is suitable for the Iranian who has Islamic national habits of praying.
4. The up-loading, bottom-discharging, the mechanical operation, reduce the labour intensity. Matching with automatic operation system and on-site dedusting technology, the working environment is better
5. Low energy consumption, it can reduce 30% for crude Mg/ton
6. Because the heat for the reduction tank are evenly, the reduction tank life is 30% longer than horizontal tank.
Main Technical Indicators
Total gas consumption: 2950Nm3
Electric consumption: 900Kwh/t (production consumption)
Labour number: 200 (including management)
Reduction tank: 0.18pcs/t Mg
Land recover: 50000m2 (whole plant including tank maker workshop)
Related Products

##### Cement Plant (rotary)

##### Cement Plant (vertical)

##### Crusher (with latest tech)

Copyright © 2026 Hebei Leadership Friends Engineering and Technology Co., Ltd All Rights Reserved.