Polyester Printing Mesh >>
Printing Mesh for Textile >>
Printing Mesh for T Shirts/Garme..
Printing Mesh for Flatbed Textil..
Printing Mesh for High-end Texti..
Printing Mesh for CDs/DVDs
Printing Mesh for Glass
Printing Mesh for Ceramics
Printing Mesh for Electronics >>
Printing Mesh for Printed Circui..
Prinitng Mesh for Membrane Switc..
Polyester/Nylon Filter Mesh
Polyester Filter Belt >>
Polyester Linear Screen
Spiral Dryer Fabric
Spiral Press Filter Belt
Sludge Dewatering Belt
Polyester Dryer Screen
Polyester Forming Fabric
Desulfurization Filter Cloth
Stainless Steel Filter Mesh >>
Square Weave Mesh >>
Stainless Steel Filter Cloth
Stainless Steel Crimped Mesh
Dutch Weave Mesh >>
Plain Dutch Weave Mesh
Twill Dutch Weave Mesh

Add: | Industrial Park Zone of South
| Anping County, Hebei Province,
| China.
Zip: | 053600
Tel: | +86-15369679157
Skype: | summerpfmscreen
E-mail: | info@pfmscreen.com
| sales@pfmscreen.com

Products
Home -> Polyester Printing Mesh -> Printing Mesh for Textile -> Printing Mesh for High-end Textile

## Printing Mesh for High-end Textile

The ability of print with any ink type, full saturate front and back of the fabrics make screen printing to be one of the optimal methods for high-end textile decoration. The recommend polyester printing mesh (silk screen) for high-end textile printing mesh is higher than 200 mesh/inch.

Polyester Printing Mesh ( Silk Screen ) For High-end Textile
Model | Mesh/cm | Mesh/Inch | Aperture (μm) | Thread Dia. (μm) | Open Area (%) | Thickness (μm) | Theoretical Ink (cm3/m2)
64-55 | 64 | 160 | 98 | 55 | 38 | 98 | 36
64-64 | 64 | 160 | 85 | 64 | 30 | 115 | 34
68-55 | 68 | 175 | 85 | 55 | 34 | 85 | 28
68-64 | 68 | 175 | 78 | 64 | 28 | 105 | 30
72-48 | 72 | 182 | 90 | 48 | 36 | 78 | 33
72-55 | 72 | 182 | 85 | 55 | 30 | 90 | 27
80-48 | 80 | 200 | 72 | 48 | 33 | 74 | 25
90-48 | 90 | 230 | 56 | 48 | 25 | 78 | 19
100-40 | 100 | 255 | 58 | 40 | 33 | 63 | 21
110-40 | 110 | 280 | 48 | 40 | 27 | 64 | 17
120-31 | 120 | 305 | 49 | 31 | 35 | 49 | 17
120-34 | 120 | 305 | 45 | 34 | 30 | 55 | 16
Note:The above theoretic data is for reference only, and thickness tollerance is ±5%.