Polyester Printing Mesh >>
Printing Mesh for Textile >>
Printing Mesh for T Shirts/Garme..
Printing Mesh for Flatbed Textil..
Printing Mesh for High-end Texti..
Printing Mesh for CDs/DVDs
Printing Mesh for Glass
Printing Mesh for Ceramics
Printing Mesh for Electronics >>
Printing Mesh for Printed Circui..
Prinitng Mesh for Membrane Switc..
Polyester/Nylon Filter Mesh
Polyester Filter Belt >>
Polyester Linear Screen
Spiral Dryer Fabric
Spiral Press Filter Belt
Sludge Dewatering Belt
Polyester Dryer Screen
Polyester Forming Fabric
Desulfurization Filter Cloth
Stainless Steel Filter Mesh >>
Square Weave Mesh >>
Stainless Steel Filter Cloth
Stainless Steel Crimped Mesh
Dutch Weave Mesh >>
Plain Dutch Weave Mesh
Twill Dutch Weave Mesh

Add: | Industrial Park Zone of South
| Anping County, Hebei Province,
| China.
Zip: | 053600
Tel: | +86-15369679157
Skype: | summerpfmscreen
E-mail: | info@pfmscreen.com
| sales@pfmscreen.com

Products
Home -> Polyester Filter Belt -> Polyester Forming Fabric

## Polyester Forming Fabric

According to the weaving, polyester forming fabric can be divided into 4-shed single-layer fabric, 5-shed single-layer fabric, 8-shed single-layer fabric, 7-shed double-layer fabric, 8-shed two and a half layer fabric, 16-shed two and a half layer fabric etc.

4-shed single-layer forming fabric is standard type of polyester forming fabric in paper making, which is suit for hygienic paper, cultural printing paper, packing paper and so on.
5-shed single-layer forming fabric is suit for hygienic paper, cultural printing paper and packing paper, etc.
8-shed single-layer forming fabric is the most wear-resisiting one in the single-layer series, with long performance life and relatively deep wire mark on the paper. It is mainly used to make the paper for paper bag, kraft paper, cardboard and corrugated paper, etc.
7-shed double-layer forming fabric is suit for high quality printing paper and tissue paper, etc.
8-shed double-layer forming fabric is suit for high quality printing paper and tissue paper, etc.
8-shed, 16-shed two and a half layer fabric is suit for high quality printing paper and various kinds of paper.
Multi - shed three-layer fabric is suit for high quality printing paper, tissue paper and cigarette paper, etc.

Polyester Forming Fabric
Weaving Types | Model | Thread Dia. (mm) | Density (No.s/cm) | Srength (N/cm) | Thickness (mm) | Air Permeability (m ³/m ² h)
Warp | Weft | Warp | Weft
4-shed single-layer fabric | 27254 | 0.2 | 0.25 | 30 | 22 | ≧600 | 0.49 | 8000
27254-1 | 0.2 | 0.25 | 30 | 23 | ≧600 | 0.495 | 7500
27254-2 | 0.2 | 0.25 | 30 | 24 | ≧600 | 0.50 | 7000
27274 | 0.2 | 0.27 | 30 | 21.5 | ≧600 | 0.51 | 7800
27274-1 | 0.2 | 0.27 | 30 | 22.5 | ≧600 | 0.515 | 7300
31204 | 0.18 | 0.2 | 35 | 28 | ≧600 | 0.43 | 7500
31204-1 | 0.18 | 0.2 | 35 | 30 | ≧600 | 0.43 | 7000
31204-2 | 0.18 | 0.2 | 35 | 30.5 | ≧600 | 0.43 | 6500
5-shed single-layer fabric | 28205 | 0.2 | 0.2 | 30 | 27.5 | ≧600 | 0.46 | 6800
30205 | 0.17 | 0.2 | 32 | 28.5 | ≧500 | 0.41 | 7100
30175 | 0.17 | 0.17 | 32 | 29.5 | ≧500 | 0.39 | 6600
31215 | 0.2 | 0.21 | 35 | 32 | ≧600 | 0.48 | 7000
8-shed single-layer fabric | 25358 | 0.22 | 0.35 | 28 | 19.5 | ≧700 | 0.85 | 9000
25388 | 0.22 | 0.38 | 29.5 | 19 | ≧700 | 0.87 | 8500
27358 | 0.22 | 0.35 | 29 | 20 | ≧700 | 0.85 | 8500
27388 | 0.22 | 0.38 | 31.5 | 19 | ≧700 | 0.87 | 8000
7-shed double-layer fabric | 50207 | 0.2 | 0.20/0.22 | 54.7 | 36.6 | ≧800 | 0.71 | 5800
0.22(t66)
56177 | 0.17 | 0.17/0.20 | 60 | 48 | ≧800 | 0.635 | 5200
0.20(t66)
57177 | 0.17 | 0.17/0.22 | 65.7 | 49.6 | ≧800 | 0.635 | 4550
0.22(t66)
64177 | 0.15 | 0.17/0.17 | 70 | 50 | ≧800 | 0.59 | 5200
0.17(t66)
8-shed double-layer fabric | 56188 | 0.17 | 0.18/0.20 | 61.3 | 51.2 | ≧850 | 0.65 | 5700
0.20(t66)
60188 | 0.18 | 0.19/0.20 | 66 | 49 | ≧900 | 0.68 | 4750
0.20(t66)
62188 | 0.15 | 0.16/0.19 | 70.5 | 50.5 | ≧900 | 0.60 | 6200
0.19(t66)

Weaving Types | Model | Thread Dia. (mm) | Density (No.s/cm) | Air Permeability (m ³/m ² h)
Warp | Weft (top/bottom) | Warp | Weft
16-shed two and a half layer fabric | CXW324016 | 0.28 | 0.20,0.27/0.40,0.40 | 37-38 | 40-41 | 6000
CXW344156 | 0.28 | 0.20,0.27/0.45,0.45 | 37-38 | 31-32 | 6000
CXW384016 | 0.22 | 0.22,0.27/0.40,0.40 | 43-44 | 40-41 | 7500
CXW434106-1 | 0.20 | 0.20,0.25/0.40,0.40 | 48-49 | 42-43 | 7000
CXW434106-2 | 0.20 | 0.20,0.25/0.40,0.40 | 48-49 | 45-46 | 6200
CXW602016-1 | 0.17 | 0.13,0.17/0.20,0.20 | 68-69 | 57-58 | 5500
CXW602016-2 | 0.17 | 0.13,0.17/0.20,0.20 | 38-69 | 61-62 | 5600
CXW603216-1 | 0.17 | 0.13,0.18/0.23,0.23 | 68-69 | 55-56 | 6000
CXW603216-2 | 0.17 | 0.13,0.18/0.23,0.23 | 68-69 | 55-56 | 6500
CXW602516-1 | 0.17 | 0.13,0.18/0.25,0.25 | 68-69 | 51-52 | 6500
CXW602516-2 | 0.17 | 0.13,0.18/0.25,0.25 | 68-69 | 61-62 | 4200
CXW603016-1 | 0.17 | 0.13,0.20/0.30,0.30 | 68-69 | 55-56 | 5000
CXW603016-2 | 0.17 | 0.13,0.20/0.30,0.30 | 68-69 | 58-59 | 4200
CXW603516 | 0.17 | 0.13,0.20/0.35,0.35 | 68-69 | 46-47 | 7500
CXW603516-1 | 0.17 | 0.13,0.20/0.35,0.35 | 68-69 | 49-50 | 6500
CXW603516-2 | 0.17 | 0.13,0.20/0.35,0.35 | 68-69 | 52-53 | 5500
CXW603516-3 | 0.17 | 0.13,0.20/0.35,0.35 | 68-69 | 54-55 | 5000
CXW603516-4 | 0.17 | 0.13,0.20/0.35,0.35 | 68-69 | 55-56 | 4500
CXW603516-5 | 0.17 | 0.13,0.20/0.35,0.35 | 68-69 | 56-57 | 4000