Polyester Filter Belt >>
Polyester Linear Screen
Spiral Dryer Fabric
Spiral Press Filter Belt
Sludge Dewatering Belt
Polyester Dryer Screen
Polyester Forming Fabric
Desulfurization Filter Cloth
Polyester Printing Mesh >>
Printing Mesh for Textile >>
Printing Mesh for T Shirts/Garme..
Printing Mesh for Flatbed Textil..
Printing Mesh for High-end Texti..
Printing Mesh for CDs/DVDs
Printing Mesh for Glass
Printing Mesh for Ceramics
Printing Mesh for Electronics >>
Printing Mesh for Printed Circui..
Prinitng Mesh for Membrane Switc..
Polyester/Nylon Filter Mesh
Stainless Steel Filter Mesh >>
Square Weave Mesh
Dutch Weave Mesh

Add: | Industrial Park Zone of South
| Anping County, Hebei Province,
| China.
Zip: | 053600
Tel: | +86-15369679157
Skype: | summerpfmscreen
E-mail: | info@pfmscreen.com
| sales@pfmscreen.com

Products
Home-> Polyester Printing Mesh -> Printing Mesh for Electronics -> Prinitng Mesh for Membrane Switches

## Prinitng Mesh for Membrane Switches

- 1
- 37591341200195
- probim_2011030218374734

Recently membrane switches are widely used to connect devices, such as cell phones, remote controls, calculators, machine controls, microwave ovens and other kitchen appliances. And screen printing is commonly used to print the conductive switch lines and the adhesive layers during the membrane switches production.

Polyester Printing Mesh ( Screen Printing Mesh ) For Membrane Switches
Model | Mesh/cm | Mesh/Inch | Aperture (μ m) | Thread Dia. (μ m) | Open Area (%) | Thickness (μ m) | Theoretical Ink (cm3/m2)
72-48 | 72 | 182 | 90 | 48 | 36 | 78 | 33
72-55 | 72 | 182 | 85 | 55 | 30 | 90 | 27
80-48 | 80 | 200 | 72 | 48 | 33 | 74 | 25
90-48 | 90 | 230 | 56 | 48 | 25 | 78 | 19
100-40 | 100 | 255 | 58 | 40 | 33 | 63 | 21
110-40 | 110 | 280 | 48 | 40 | 27 | 64 | 17
120-31 | 120 | 305 | 49 | 31 | 35 | 49 | 17
120-34 | 120 | 305 | 45 | 34 | 30 | 55 | 16
130-34 | 130 | 330 | 40 | 34 | 27 | 55 | 15
140-31 | 140 | 355 | 36 | 31 | 26 | 48 | 12
140-34 | 140 | 355 | 31 | 34 | 20 | 53 | 10
150-31 | 150 | 380 | 32 | 31 | 23 | 49 | 11
150-34 | 150 | 380 | 23 | 34 | 13 | 55 | 6.5
165-31 | 165 | 420 | 23 | 31 | 15 | 48 | 7
180-27 | 180 | 460 | 22 | 27 | 15.1 | 43 | 6.5
180-31 | 180 | 460 | 23 | 31 | 16.5 | 56 | 9.3
Note:The above theoretic data is for reference only,and thickness tollerance is±5%.