Polyester Printing Mesh >>
Printing Mesh for Textile >>
Printing Mesh for T Shirts/Garme..
Printing Mesh for Flatbed Textil..
Printing Mesh for High-end Texti..
Printing Mesh for CDs/DVDs
Printing Mesh for Glass
Printing Mesh for Ceramics
Printing Mesh for Electronics >>
Printing Mesh for Printed Circui..
Prinitng Mesh for Membrane Switc..
Polyester/Nylon Filter Mesh
Polyester Filter Belt >>
Polyester Linear Screen
Spiral Dryer Fabric
Spiral Press Filter Belt
Sludge Dewatering Belt
Polyester Dryer Screen
Polyester Forming Fabric
Desulfurization Filter Cloth
Stainless Steel Filter Mesh >>
Square Weave Mesh >>
Stainless Steel Filter Cloth
Stainless Steel Crimped Mesh
Dutch Weave Mesh >>
Plain Dutch Weave Mesh
Twill Dutch Weave Mesh

Add: | Industrial Park Zone of South
| Anping County, Hebei Province,
| China.
Zip: | 053600
Tel: | +86-15369679157
Skype: | summerpfmscreen
E-mail: | info@pfmscreen.com
| sales@pfmscreen.com

Products
Home-> Polyester Printing Mesh -> Printing Mesh for Textile -> Printing Mesh for T Shirts/Garments

## Printing Mesh for T Shirts/Garments

Screen printing can transfer thick ink deposits and creat special effects to make it to be optimal process to print high quality commercial garment.

From 30 mesh/inch to 300 mesh/inch of polyester printing mesh (bolting cloth) is commonly aplied to T shirts/garments printing.

Polyester Printing Mesh (Bolting Cloth) For T Shirts/Garments
Model | Mesh/cm | Mesh/Inch | Aperture (μ m) | Thread Dia. (μ m) | Open Area (%) | Thickness (μ m) | Theoretical Ink (cm3/m2)
12-140 | 12 | 30 | 686 | 140 | 68 | 277 | 189
13-150 | 13 | 33 | 619 | 150 | 64 | 300 | 128
16-140 | 16 | 40 | 461 | 140 | 58 | 238 | 139
21-80 | 21 | 55 | 296 | 80 | 69 | 120 | 79
21-150 | 21 | 55 | 326 | 150 | 46 | 260 | 118
22-80 | 22 | 56 | 356 | 80 | 66 | 136 | 90
24-80 | 24 | 60 | 320 | 80 | 63 | 136 | 86
24-100 | 24 | 60 | 316 | 100 | 57 | 170 | 65
28-140 | 28 | 70 | 217 | 140 | 40 | 195 | 76
32-55 | 32 | 80 | 257 | 55 | 67 | 103 | 67
32-64 | 32 | 80 | 248 | 64 | 63 | 95 | 56
32-100 | 32 | 80 | 212 | 100 | 46 | 170 | 73
36-90 | 36 | 92 | 183 | 90 | 44 | 150 | 65
39-55 | 39 | 100 | 177 | 55 | 56 | 88 | 55
43-80 | 43 | 110 | 149 | 80 | 41 | 130 | 53
47-55 | 47 | 120 | 152 | 55 | 51 | 88 | 48
48-70 | 48 | 122 | 133 | 70 | 41 | 115 | 47
53-55 | 53 | 135 | 133 | 55 | 50 | 86 | 42
54-64 | 54 | 137 | 115 | 64 | 39 | 100 | 39
54-70 | 54 | 137 | 109 | 70 | 35 | 116 | 40
61-64 | 61 | 155 | 90 | 64 | 31 | 101 | 30
64-55 | 64 | 160 | 98 | 55 | 38 | 98 | 36
64-64 | 64 | 160 | 85 | 64 | 30 | 115 | 34
68-55 | 68 | 175 | 85 | 55 | 34 | 85 | 28
68-64 | 68 | 175 | 78 | 64 | 28 | 105 | 30
72-48 | 72 | 182 | 90 | 48 | 36 | 78 | 33
72-55 | 72 | 182 | 85 | 55 | 30 | 90 | 27
80-48 | 80 | 200 | 72 | 48 | 33 | 74 | 25
90-48 | 90 | 230 | 56 | 48 | 25 | 78 | 19
100-40 | 100 | 255 | 58 | 40 | 33 | 63 | 21
110-40 | 110 | 280 | 48 | 40 | 27 | 64 | 17
120-31 | 120 | 305 | 49 | 31 | 35 | 49 | 17
120-34 | 120 | 305 | 45 | 34 | 30 | 55 | 16
Note:The above theoretic data is for reference only,and thickness tollerance is±5%.