Polyester Filter Belt >>
Polyester Linear Screen
Spiral Dryer Fabric
Spiral Press Filter Belt
Sludge Dewatering Belt
Polyester Dryer Screen
Polyester Forming Fabric
Desulfurization Filter Cloth
Polyester Printing Mesh >>
Printing Mesh for Textile >>
Printing Mesh for T Shirts/Garme..
Printing Mesh for Flatbed Textil..
Printing Mesh for High-end Texti..
Printing Mesh for CDs/DVDs
Printing Mesh for Glass
Printing Mesh for Ceramics
Printing Mesh for Electronics >>
Printing Mesh for Printed Circui..
Prinitng Mesh for Membrane Switc..
Polyester/Nylon Filter Mesh
Stainless Steel Filter Mesh >>
Square Weave Mesh
Dutch Weave Mesh

Add: | Industrial Park Zone of South
| Anping County, Hebei Province,
| China.
Zip: | 053600
Tel: | +86-15369679157
Skype: | summerpfmscreen
E-mail: | info@pfmscreen.com
| sales@pfmscreen.com

Products
Home-> Polyester Printing Mesh -> Printing Mesh for Textile -> Printing Mesh for Flatbed Textile

## Printing Mesh for Flatbed Textile

- 1
- 2
- 3

With flatbed textile printing, any ink deposits and any ink systerm are possible with lager range of width. In this field, polyester printing mesh (polyester printing screen) can used to print knitted fabric, blankets, chiffon silk even coarse denim. Now the width of our polyester printing screen for textile is up to 145 inch.

Polyester Printing Mesh ( Bolting Cloth ) For Flatbed Textile
Model | Mesh/cm | Mesh/Inch | Aperture (μ m) | Thread Dia. (μ m) | Open Area (%) | Thickness (μ m) | Theoretical Ink (cm3/m2)
12-140 | 12 | 30 | 686 | 140 | 68 | 277 | 189
13-150 | 13 | 33 | 619 | 150 | 64 | 300 | 128
16-140 | 16 | 40 | 461 | 140 | 58 | 238 | 139
21-80 | 21 | 55 | 296 | 80 | 69 | 120 | 79
21-150 | 21 | 55 | 326 | 150 | 46 | 260 | 118
22-80 | 22 | 56 | 356 | 80 | 66 | 136 | 90
24-80 | 24 | 60 | 320 | 80 | 63 | 136 | 86
24-100 | 24 | 60 | 316 | 100 | 57 | 170 | 65
28-140 | 28 | 70 | 217 | 140 | 40 | 195 | 76
32-55 | 32 | 80 | 257 | 55 | 67 | 103 | 67
32-64 | 32 | 80 | 248 | 64 | 63 | 95 | 56
32-100 | 32 | 80 | 212 | 100 | 46 | 170 | 73
36-90 | 36 | 92 | 183 | 90 | 44 | 150 | 65
39-55 | 39 | 100 | 177 | 55 | 56 | 88 | 55
43-80 | 43 | 110 | 149 | 80 | 41 | 130 | 53
47-55 | 47 | 120 | 152 | 55 | 51 | 88 | 48
48-70 | 48 | 122 | 133 | 70 | 41 | 115 | 47
53-55 | 53 | 135 | 133 | 55 | 50 | 86 | 42
54-64 | 54 | 137 | 115 | 64 | 39 | 100 | 39
54-70 | 54 | 137 | 109 | 70 | 35 | 116 | 40
61-64 | 61 | 155 | 90 | 64 | 31 | 101 | 30
64-55 | 64 | 160 | 98 | 55 | 38 | 98 | 36
64-64 | 64 | 160 | 85 | 64 | 30 | 115 | 34
68-55 | 68 | 175 | 85 | 55 | 34 | 85 | 28
68-64 | 68 | 175 | 78 | 64 | 28 | 105 | 30
72-48 | 72 | 182 | 90 | 48 | 36 | 78 | 33
72-55 | 72 | 182 | 85 | 55 | 30 | 90 | 27
80-48 | 80 | 200 | 72 | 48 | 33 | 74 | 25
90-48 | 90 | 230 | 56 | 48 | 25 | 78 | 19
100-40 | 100 | 255 | 58 | 40 | 33 | 63 | 21
110-40 | 110 | 280 | 48 | 40 | 27 | 64 | 17
120-31 | 120 | 305 | 49 | 31 | 35 | 49 | 17
120-34 | 120 | 305 | 45 | 34 | 30 | 55 | 16
Note:The above theoretic data is for reference only, and thickness tollerance is±5%.