Polyester Printing Mesh >>
Printing Mesh for Textile >>
Printing Mesh for T Shirts/Garme..
Printing Mesh for Flatbed Textil..
Printing Mesh for High-end Texti..
Printing Mesh for CDs/DVDs
Printing Mesh for Glass
Printing Mesh for Ceramics
Printing Mesh for Electronics >>
Printing Mesh for Printed Circui..
Prinitng Mesh for Membrane Switc..
Polyester/Nylon Filter Mesh
Polyester Filter Belt >>
Polyester Linear Screen
Spiral Dryer Fabric
Spiral Press Filter Belt
Sludge Dewatering Belt
Polyester Dryer Screen
Polyester Forming Fabric
Desulfurization Filter Cloth
Stainless Steel Filter Mesh >>
Square Weave Mesh >>
Stainless Steel Filter Cloth
Stainless Steel Crimped Mesh
Dutch Weave Mesh >>
Plain Dutch Weave Mesh
Twill Dutch Weave Mesh

Add: | Industrial Park Zone of South
| Anping County, Hebei Province,
| China.
Zip: | 053600
Tel: | +86-15369679157
Skype: | summerpfmscreen
E-mail: | info@pfmscreen.com
| sales@pfmscreen.com

Products
Home -> Polyester Printing Mesh -> Printing Mesh for Glass

## Printing Mesh for Glass

1.Pharmacy Glass Appliance Printing
Direct screen printing on articles for pharmacy glass appliance, such as appliance name, measuring marks.

2.Home Appliance Printing
Print the glass decorations on household appliances such as microwaves oven doors and ceramic hot plates/stove tops.

3.Automotive Glass Printing
The black mask for the front, side and back windows, heating patterns, antennas (radio, GPS)and sun roofs.

4.Glass Containers Printing
Perfumes, cosmetics and drink bottles are decorated with screen printing methods.

Polyester Printing Mesh ( Silk Screen Printing Mesh ) For Glass
Model | Mesh/cm | Mesh/Inch | Aperture (μm) | Thread Dia. (μm) | Open Area (%) | Thickness (μm) | Theoretical Ink (cm3/m2)
36-90 | 36 | 92 | 183 | 90 | 44 | 150 | 65
39-55 | 39 | 100 | 177 | 55 | 56 | 88 | 55
43-80 | 43 | 110 | 149 | 80 | 41 | 130 | 53
47-55 | 47 | 120 | 152 | 55 | 51 | 88 | 48
48-70 | 48 | 122 | 133 | 70 | 41 | 115 | 47
53-55 | 53 | 135 | 133 | 55 | 50 | 86 | 42
54-64 | 54 | 137 | 115 | 64 | 39 | 100 | 39
54-70 | 54 | 137 | 109 | 70 | 35 | 116 | 40
61-64 | 61 | 155 | 90 | 64 | 31 | 101 | 30
64-55 | 64 | 160 | 98 | 55 | 38 | 98 | 36
64-64 | 64 | 160 | 85 | 64 | 30 | 115 | 34
68-55 | 68 | 175 | 85 | 55 | 34 | 85 | 28
68-64 | 68 | 175 | 78 | 64 | 28 | 105 | 30
72-48 | 72 | 182 | 90 | 48 | 36 | 78 | 33
72-55 | 72 | 182 | 85 | 55 | 30 | 90 | 27
80-48 | 80 | 200 | 72 | 48 | 33 | 74 | 25
90-48 | 90 | 230 | 56 | 48 | 25 | 78 | 19
100-40 | 100 | 255 | 58 | 40 | 33 | 63 | 21
110-40 | 110 | 280 | 48 | 40 | 27 | 64 | 17
120-31 | 120 | 305 | 49 | 31 | 35 | 49 | 17
120-34 | 120 | 305 | 45 | 34 | 30 | 55 | 16
130-34 | 130 | 330 | 40 | 34 | 27 | 55 | 15
140-31 | 140 | 355 | 36 | 31 | 26 | 48 | 12
140-34 | 140 | 355 | 31 | 34 | 20 | 53 | 10
150-31 | 150 | 380 | 32 | 31 | 23 | 49 | 11
150-34 | 150 | 380 | 23 | 34 | 13 | 55 | 6.5
165-31 | 165 | 420 | 23 | 31 | 15 | 48 | 7
Note: The above theoretic data is for reference only, and thickness tollerance is±5%.