Polyester Printing Mesh >>
Printing Mesh for Textile >>
Printing Mesh for T Shirts/Garme..
Printing Mesh for Flatbed Textil..
Printing Mesh for High-end Texti..
Printing Mesh for CDs/DVDs
Printing Mesh for Glass
Printing Mesh for Ceramics
Printing Mesh for Electronics >>
Printing Mesh for Printed Circui..
Prinitng Mesh for Membrane Switc..
Polyester/Nylon Filter Mesh
Polyester Filter Belt >>
Polyester Linear Screen
Spiral Dryer Fabric
Spiral Press Filter Belt
Sludge Dewatering Belt
Polyester Dryer Screen
Polyester Forming Fabric
Desulfurization Filter Cloth
Stainless Steel Filter Mesh >>
Square Weave Mesh >>
Stainless Steel Filter Cloth
Stainless Steel Crimped Mesh
Dutch Weave Mesh >>
Plain Dutch Weave Mesh
Twill Dutch Weave Mesh

Add: | Industrial Park Zone of South
| Anping County, Hebei Province,
| China.
Zip: | 053600
Tel: | +86-15369679157
Skype: | summerpfmscreen
E-mail: | info@pfmscreen.com
| sales@pfmscreen.com

Products
Home -> Stainless Steel Filter Mesh -> Square Weave Mesh -> Stainless Steel Crimped Mesh

## Stainless Steel Crimped Mesh

Features of stainless crimped mesh:
Material: low carbon steel wire, SS304. 304L, 316, 316L, brass wire, etc.
Crimped mesh is woven after crimping, so it firm and dutable with beautiful outlook.
Applications of Crimped Mesh:
Stainless steel crimped mesh is mainly used in screening in mine, coal industry, construction, oasting of flour food and meat, etc.

Crimped Mesh
Wire Gauge (BWG) | Aperture Size (mm) | Wire Dia. (mm) | Weight(Kg/m²)
8 | 30 | 4.06 | 6.00
8 | 25 | 4.06 | 7.00
8 | 20 | 4.06 | 8.00
8 | 15 | 4.06 | 1.00
8 | 12 | 4.06 | 13.00
8 | 10 | 4.06 | 15.00
10 | 30 | 3.25 | 4.00
10 | 25 | 3.25 | 4.70
10 | 20 | 3.25 | 5.80
10 | 15 | 3.25 | 7.40
10 | 10 | 3.25 | 10.00
12 | 30 | 2.64 | 2.70
12 | 12 | 2.64 | 3.20
12 | 20 | 2.64 | 3.90
12 | 15 | 2.64 | 5.00
12 | 10 | 2.64 | 7.00
14 | 20 | 2.03 | 2.38
14 | 15 | 2.03 | 3.10
14 | 12 | 2.03 | 3.70
14 | 10 | 2.03 | 4.35
14 | 8 | 2.03 | 5.22
14 | 6 | 2.03 | 6.52
14 | 4 | 2.03 | 8.68
14 | 3 | 2.03 | 10.40
16 | 15 | 1.63 | 2.03
16 | 10 | 1.63 | 2.90
16 | 8 | 1.63 | 3.50
16 | 6 | 1.63 | 4.40
16 | 4 | 1.63 | 5.99
18 | 12 | 1.22 | 1.43
18 | 10 | 1.22 | 1.68
18 | 8 | 1.22 | 2.05
18 | 6 | 1.22 | 2.62
18 | 4 | 1.22 | 3.62
18 | 3 | 1.22 | 4.48
20 | 12 | 0.91 | 0.82
20 | 10 | 0.91 | 0.96
20 | 8 | 0.91 | 1.18
20 | 5 | 0.91 | 1.78
20 | 4 | 0.91 | 2.15
20 | 3 | 0.91 | 2.69