Polyester Filter Belt >>
Polyester Linear Screen
Spiral Dryer Fabric
Spiral Press Filter Belt
Sludge Dewatering Belt
Polyester Dryer Screen
Polyester Forming Fabric
Desulfurization Filter Cloth
Polyester Printing Mesh >>
Printing Mesh for Textile >>
Printing Mesh for T Shirts/Garme..
Printing Mesh for Flatbed Textil..
Printing Mesh for High-end Texti..
Printing Mesh for CDs/DVDs
Printing Mesh for Glass
Printing Mesh for Ceramics
Printing Mesh for Electronics >>
Printing Mesh for Printed Circui..
Prinitng Mesh for Membrane Switc..
Polyester/Nylon Filter Mesh
Stainless Steel Filter Mesh >>
Square Weave Mesh
Dutch Weave Mesh

Add: | Industrial Park Zone of South
| Anping County, Hebei Province,
| China.
Zip: | 053600
Tel: | +86-15369679157
Skype: | summerpfmscreen
E-mail: | info@pfmscreen.com
| sales@pfmscreen.com

Products
Home-> Polyester Printing Mesh -> Printing Mesh for Electronics -> Printing Mesh for Printed Circuit Boards

## Printing Mesh for Printed Circuit Boards

- DSC_0377
- PCB线路板
- SAM_0954

Screen printing is the fastest and most economical method to print printed circuit boards (PCB) solder masks, etching resist, legends and single or multi-layers.

Polyester Printing Mesh ( Screen Printing Mesh ) For PCB
Model | Mesh/cm | Mesh/Inch | Aperture (μ m) | Thread Dia. (μ m) | Open Area (%) | Thickness (μ m) | Theoretical Ink (cm3/m2)
43-80 | 43 | 110 | 149 | 80 | 41 | 130 | 53
47-55 | 47 | 120 | 152 | 55 | 51 | 88 | 48
48-70 | 48 | 122 | 133 | 70 | 41 | 115 | 47
53-55 | 53 | 135 | 133 | 55 | 50 | 86 | 42
54-64 | 54 | 137 | 115 | 64 | 39 | 100 | 39
54-70 | 54 | 137 | 109 | 70 | 35 | 116 | 40
61-64 | 61 | 155 | 90 | 64 | 31 | 101 | 30
64-55 | 64 | 160 | 98 | 55 | 38 | 98 | 36
64-64 | 64 | 160 | 85 | 64 | 30 | 115 | 34
68-55 | 68 | 175 | 85 | 55 | 34 | 85 | 28
68-64 | 68 | 175 | 78 | 64 | 28 | 105 | 30
72-48 | 72 | 182 | 90 | 48 | 36 | 78 | 33
72-55 | 72 | 182 | 85 | 55 | 30 | 90 | 27
80-48 | 80 | 200 | 72 | 48 | 33 | 74 | 25
90-48 | 90 | 230 | 56 | 48 | 25 | 78 | 19
100-40 | 100 | 255 | 58 | 40 | 33 | 63 | 21
110-40 | 110 | 280 | 48 | 40 | 27 | 64 | 17
120-31 | 120 | 305 | 49 | 31 | 35 | 49 | 17
120-34 | 120 | 305 | 45 | 34 | 30 | 55 | 16
130-34 | 130 | 330 | 40 | 34 | 27 | 55 | 15
140-31 | 140 | 355 | 36 | 31 | 26 | 48 | 12
140-34 | 140 | 355 | 31 | 34 | 20 | 53 | 10
150-31 | 150 | 380 | 32 | 31 | 23 | 49 | 11
150-34 | 150 | 380 | 23 | 34 | 13 | 55 | 6.5
165-31 | 165 | 420 | 23 | 31 | 15 | 48 | 7
Note:The above theoretic data is for reference only, and thickness tollerance is ±5%.