Polyester Printing Mesh >>
Printing Mesh for Textile >>
Printing Mesh for T Shirts/Garme..
Printing Mesh for Flatbed Textil..
Printing Mesh for High-end Texti..
Printing Mesh for CDs/DVDs
Printing Mesh for Glass
Printing Mesh for Ceramics
Printing Mesh for Electronics >>
Printing Mesh for Printed Circui..
Prinitng Mesh for Membrane Switc..
Polyester/Nylon Filter Mesh
Polyester Filter Belt >>
Polyester Linear Screen
Spiral Dryer Fabric
Spiral Press Filter Belt
Sludge Dewatering Belt
Polyester Dryer Screen
Polyester Forming Fabric
Desulfurization Filter Cloth
Stainless Steel Filter Mesh >>
Square Weave Mesh >>
Stainless Steel Filter Cloth
Stainless Steel Crimped Mesh
Dutch Weave Mesh >>
Plain Dutch Weave Mesh
Twill Dutch Weave Mesh

Add: | Industrial Park Zone of South
| Anping County, Hebei Province,
| China.
Zip: | 053600
Tel: | +86-15369679157
Skype: | summerpfmscreen
E-mail: | info@pfmscreen.com
| sales@pfmscreen.com

Products
Home-> Polyester Printing Mesh -> Printing Mesh for CDs/DVDs

## Printing Mesh for CDs/DVDs

Screen printing offers many superiorities of ink transparency, ink briliance, various decorative pattern choice, and the most important is the fast production cycle time and unaffected disc performance. So screen printing is the perferred printing process for CDs and DVDs decoration.

The most widely used mesh/count of polyester printing screen for CDs/DVDs is higher than 230 mesh/inch.

Polyester Printing Mesh ( Polyester Printing Screen ) For CDs/DVDs
Model | Mesh/cm | Mesh/inch | Aperture (μm) | Thread Dia. (μm) | Open Area (%) | Thickness (μm) | Theoretical Ink (cm3/m2)
72-48 | 72 | 182 | 90 | 48 | 36 | 78 | 33
72-55 | 72 | 182 | 85 | 55 | 30 | 90 | 27
80-48 | 80 | 200 | 72 | 48 | 33 | 74 | 25
90-48 | 90 | 230 | 56 | 48 | 25 | 78 | 19
100-40 | 100 | 255 | 58 | 40 | 33 | 63 | 21
110-40 | 110 | 280 | 48 | 40 | 27 | 64 | 17
120-31 | 120 | 305 | 49 | 31 | 35 | 49 | 17
120-34 | 120 | 305 | 45 | 34 | 30 | 55 | 16
130-34 | 130 | 330 | 40 | 34 | 27 | 55 | 15
140-31 | 140 | 355 | 36 | 31 | 26 | 48 | 12
140-34 | 140 | 355 | 31 | 34 | 20 | 53 | 10
150-31 | 150 | 380 | 32 | 31 | 23 | 49 | 11
150-34 | 150 | 380 | 23 | 34 | 13 | 55 | 6.5
165-31 | 165 | 420 | 23 | 31 | 15 | 48 | 7
180-27 | 180 | 460 | 22 | 27 | 15.1 | 43 | 6.5
180-31 | 180 | 460 | 23 | 31 | 16.5 | 56 | 9.3
Note:The above theoretic data is for reference only, and thickness tollerance is ±5%.