mini electric winch
https://www.liftingcn.com/electric-hoist-and-winch/mini-electric-winch/

Product Details:Fast Line Speed Electric Winch for Construction
1.The  gearbox case of the winch was made of high-strength aluminum alloy materials with light weight and high precision.

2. The high speed winch increased the module gear which could reduce the noise of the gearbox ,higher safety coefficient and longer use time.

3.The mini electric winch equiped with  afterburner system,specific motor,case fan,the rotary steel wire rope,Rotating hook and so on.The configuration is very high.

4.The construction winch looks delicate appearance and high grade.

Fast Line Speed Electric Winch for Construction
Items\Types
DTS-200-100-A
DTS-300-100-A
DTS-400-100-A
DTS-500-100-A
Loading Weight(kg)
single rope:200kg
double rope:400kg
single rope:300kg
double rope:600kg
single rope:400kg
double rope:800kg
single rope:500kg
double  rope:1000kg
The length of steel wire rope(m)
25m
25m
25m
25m
Lifting Speed(m/min)
10m-20m
10m-20m
6m-12m
6-12m
Motor Capacity(kw)
1.85kw
2.3kw
1.85kw
2.3kw
Supply Voltage(v)
220v
220v
220v
220v
Rope Diameter(mm)
5.0mm
6.0mm
6.0mm
7.0mm
Total Weight(kg)
33kg
38kg
35kg
40kg
Detailed Images

The steel wire rope:

The steel wire rope adopts type of 19*7 galvanized airline anti-rotation steel wire rope to guarantee the goods not to rotate during lifting .


The gearbox case of the winch:

The gearbox case of the easy to use winch was made of high-strength aluminum alloy materials with light weight and high precision.The hoist adopts the 220v big power alongside magneto motor , Which can guarantee the sensitive brake and safe use .




The module gear case:

The motor lifting winch increased the module gear which could reduce the noise of the gearbox ,higher safety coefficient and longer use time.


The power-stress button:

The power-controlled system has an innovation that it adds the power- stress button system to avoid the situation when the main engine doesn't work when the voltage is unstable or lower during the goods is lifted in mid- air.




The rotation hook:

The high-grade large -opening rotation hook ,the stress bearing is installed with the rotation bearing to guarantee the bearing can be rotated to avoid the rope wiching



The high-tension cooling fan :

It is designed and installed along the engine side to make it prefectly work.and it can meet the need of long-time working in special working please.





Product Name
Fast Line Speed Electric Winch for Construction
Voltage
110v-460v Customized
Power
2.3kw
Loading Weight
400kg-500kg
Diameter of Steel Wire Rope
6.0mm Of Galvanized Airline Anti-Rotation
Lifting Height
25m
Lifting Speed
20m/min
Color
Yellow Or Customized
Clutch
Without Clutch
OUR FACTORY PK OTHER FACTORY ABOUT THE PRODUCT DETAILS

About the below pictures, each line, the left picture belongs to other factory; the right picture belongs to our factory!



About the engine cover:
Our factory: The material of the engine cover adopts the national standard JIS H5302-2006 aluminum alloy ADC12, based on the acceptance standard of GB/T10851-1989 casting aluminum alloy pinhole.
Other factory: The material of the engine cover mostly adopts the recycling mixed aluminum. 


About the back cover of the engine:
Our factory: We adopts the ADC12 material to make the engine much more effective.
Other factory: They adopt the inferior material and rough machine.






About the gearbox case of the engine:
Our factory: The gearbox case becomes much more bigger and thicken and has a long lifespan more than 3 years. The bearings on the gearbox case also become more bigger. What's more, our factory design 2 oil-filling holes on the one side of the gearbox case so that it is convenient to fill oil and extend the lifespan of the gear usage.
Other factory: It is the old-style gearbox case which has the features of small volume, thinner case and short lifespan so that it can easily to get broken. And there is no oil-filling hole on the gearbox case, so it is not convenient to fill oil.

.



About the rotor of the engine:
Our factory: The engine rotors increase 10% in diameter and length and apply with the 600-grade sheet steel which can decrease the electricity loss so that the engine is powerful in the continuous work.
Other factory: The engine rotors are thinner and shorter and apply with the ordinary steel plate and iron plate as the raw material which can increase the electrical loss and make the engine produce heat particularly fast so that the engine has no strength in work after a short while.




About the lifting hook of the hoist:

Our factory: Ours is equipped with the 2T big hook and can rotate 360 degrees. The bigger the hook, the easier to lift the goods.
Other factory: It is the non-standard small type 0.5T hook which is not equipped with rotation function which is not easy to lift the goods. Some customers even take off it and change into the big hook to make it easy to use.


Company Information
Welcom to our factory 
 Located in Zhengzhou City, Henan Province, Mapoton is affliated to Hebei Tianyu Hoisting Machinery Manufacturing Company. It is the exclusive foreign business department of our factory.

     Our factory was established in 1993, restructured in 2006. We have stepped into the forefront of the domestic lifting industry and one of the domestic largest manufacturers in designing and producing indoor and outdoor lifting machinery, due to 20 years of accumulation and technical innovations, as well as the principles of high starting point and producing high-quality equipment. Besides, we also have been famous for manufacturing hand chain hoists, electric lifting cranes and high-altitude operation pedal baskets. 

     Over years of continuously adhering to the people-oriented and producing safe lifting equipment,. We have researched and developed full series (covering 18 categories, total 60+) indoor & outdoor hoists with payload capacity ranged 100kg-800kg. The machines secure smooth loading, safety for operators working in construction and decoration.

      Meanwhile, we have extensively developed the other types, such as stationary, portable, vehicular hoists. Moreover, we are proud of being one of the constitutors for the lifting equipment industry principles. 

      All our machines have obtained the quality inspection reports and underwritten by the CLIC(China Life Insurance Company), which is state-owned largest insurance company in China. Varieties of products have been possessed the intellectual property rights and declared the national patent. Thanks to full-blown sales network, products have been exported to Southeast Asia, Middle East. Furthermore, we have embraced a high reputation among customers. Our customer service department consists of technique support and 2-grade service system which provide professional supports in the process of pre-sale, mid-sale and after sale.

Welcome to visit our factory!




Factory Technology


Packing & Delivery









FAQ
1.Q: Are you the direct factory?
   A: Yes, we are the direct factory for 24 years even though we registered as a foreign trading company.
The address of our factory is : NO. 18 South Road, NO. 2 West Ring, Donglv Industry Zone, Qingyuan District, Baoding City, Hebei Province, China. Sincerely welcome to come and visit!
2.Q: MOQ?
   A: One set is ok.
3.Q: Can you accept payment terms?
  A: Alibaba Trade Assurance, T/T, Western Union, Credit Card, etc.
4.Q: Delivery time?
    A: If in stock,1~3 days;If not in stock,normal 5~15 days; Or according to the order.
5.Q: Warranty?
    A: One year for the electric engine. We can also provide permanent accessories repair and replacement services.
6.Q: Do your products can be customized?
  A: Yes,our all kinds of electric winch can be customized design according to each client's demands. And we can provide label and company name customized services.
7.Q: What kinds of certificates about your products?
   A: Normally,we have CE,BV,SGS,CUTR certificates,of course our products make some other certificates according to our clients' specific requirements.
8.Q: How to guarantee the quality and operation when the products leave factory?
  A: We test each parts of all products before products leave factory and guarantee the successful operation. No-test or failure-test products are prohibited leaving factory.
9.Q: We have a container in other factory or supplier, can you send cargos there?
 A: Yes, we will as long as you send us the detailed address of the place you want to send. Or it is also ok when you want to send other cargos to our factory.
10.Q: How can I get a accurate quotation?
  A: Tell and send us the product photo you want, electricity voltage, lifting height(length of the steel wire rope), lifting weight, quantities, FOB/CFR/CIF price or other detailed requirements.
11.Q: What is your HS code?
 A: 8428909090 for mini crane and aluminum electric winch; 8425110000 for mini electric hoist
12.Q: How about the installation?
 A: First, easy installation. Then, along with the cargos packages, we enclose the detailed installation and operation instructions; we can also send you the detailed installation videos.

-
Q:Whether you can offer customized crane?
A:Yep, of course, we are manufacturer, and we have our own engineer group. They can work out customized design according to your requirement. The most important thing is that you tell us what you need.


Q: Whether there is professional technician assist our installation? 
A:Yep, we have professional installation teams, who have gone to many countries to assist the installation. If you need we send technician to your factory, please let us know in advance. So we can arrange technicians.


Q: Can you help us arrange the shipment? 
A:Yep, we have professional and independent Logistics & Document department. They will be responsible for arrange the logistics. Just communicate with our sales about the destination port.


Q: How can you ensure the quality? 
A:Before delivery, every product will be made test, and we will send you the quality certification. You are also warmly welcomed to come to our factory to make inspection.

Contact Us
-
--

Find out more about Small Electric Winches from DLH Online
Small ComeUp Electric Winches

Taiwan-based specialist ComeUp have been established since 1975 and they offer a superb small electric winches which performs admirably across a range of challenging scenarios. Currently, ComeUp winches are distributed in more than 60 countries across 5 continents and they offer consumers globally the most reliable, high performance winching products and is now regarded as one of the world's most trusted names for winching solutions.

The CWL Compact Winch/Hoist is a very popular small electric winch, coming including with galvanised steel wire rope. Its lightweight and compact design ensures mobility and easy installation. Its enclosed Drum Flange prevents ropes becoming trapped between the drum and support castings whilst the dynamic and Mechanical Brake provides instant and safe braking function. All in all, it’s a dynamic winch in a small package!

As is its brand peer the CP RANGE 200-250-300-500kg Winch/Hoist, which comes in varying options with lifting capacities ranging from 250kg to 500kg. Again it’s a small electric winch that packs a punch but boasts a compact design for easy installation, not to mention its low running volume. The winch arrives complete with a 45 metre galvanised wire rope alongside a 3 metre pendant control, which is pre-wired to the winch with 2 buttons and an emergency stop function.

Small Pfaff Silberblau Electric Winches

Pfaff Silberblau are Germany-based manufacturers of material handling equipment and manufacture market-leading and highly-resilient products designed for usage in a wide range of different industrial environments.

At DLH Online, our Pfaff Silberblau small electric winches will fit the bill and as a top UK authorised distributor of Pfaff Silberblau’s parent company Columbus McKinnon, we can supply their industrial products to our customers at highly competitive prices.

For a powerful but small Pfaff Silberblau electric winches, the Pfaff Electric Wire Rope Winch Model BETA-ATEX comes highly recommended, with a starting lift capacity of 320kg. At DLH Online we proudly offer this Pfaff Silberblau electric winch with a choice of operating voltages and lifting speeds.

Small Yale Electric Winches

Alongside Pfaff Silberblau, Yale is also owned by the mammoth global Columbus McKinnon group. As DLH Online is a top UK authorised distributor for Yale equipment, we can provide Yale lifting solutions at bargain low prices to our clients.

Yale offer a fantastic small electric winch, the Yale RPE 400V or 230V Electric Wire Rope Winches - 250-1000 kg, which has a low-weight starting capacity of 250kg, is designed explicitly for performance, efficiency and safety and offer many advantages and options. The RPE‘s  extremely compact, practical cube design and universal rope lead-offs allow individual applications in virtually any position and make them very powerful aids for pulling and lifting loads.

Whatever your small electric winch requirements are, why not get in touch today and we will provide the solution!

DLH Online is the main UK authorised distributor for Thern Inc., alongside being a top UK authorised distributor for the Columbus McKinnon Group (CMCO) who incorporate the Yale, Pfaff Silberblau, Steerman and Camlok brands. DLH Online is also the Main UK-authorised distributor for Eepos, Schilling, Erikkila and Codipro. They are also the sole authorised Master UK distributors for Lifts All Sweden alongside being the main North West (UK) authorised distributors for Crosby, RUD and Donati and Sumner.  

---

The Mini Electric Pilewind winch is a compact and lightweight solution for loads up to 125 kg. Designed and manufactured in the United Kingdom it can be supplied with up to 4 ropes off the drum.

The Mini Pilewind winch is designed in accordance with BS 7906 Cat A and is suitable for the static suspension of loads without the requirement for a secondary safety device making it an ideal solution for the rigging of lighting bars, trusses and lightweight banners.

A complete range of diverter pulleys, mounting brackets and other accessories are also available upon request.

MAKE AN ENQUIRY
Technical Information
Enquire
TECHNICAL INFORMATION
The technical specification for our Mini Electric Pilewind Winches:

Robust construction
Safe working load of up to 125kg
Up to 4 ropes on a standard drum
Drum capacity of 8 meters
Operation handle included
Supplied with electrics and control box
Self sustaining gear box
415V three phase supply
Six position limit switch as standard
Mounting bracket supplied
Handle with safety interlock
Drum guard as standard

---
CE Certificate PA mini electric wire hoist is generally divided into stationary and running type, suitable for various occasions, can lift goods under 2000kg, especially suitable for lifting heavy items from downstairs of high-rise buildings.

This kind hoists has many features, such as simple structure, easy installation, small and exquisite, and use single power supply as its electricity. Mini electric hoists have reached the international standard in terms of production design and make sure of its security when using, using cast iron structure of motor cooling fin improves the service life.

Mini electric hoist lifting speed can reach up to 10 m/min, steel wire rope at the beginning of design can reach up to 12 meters long (lengthening can be customized), in terms of hook, specially designed as the advanced double Settings, greatly increased the mini electric hoist lifting weight, mini electric hoist can be used on 220V power supply, especially suitable for daily civilian, industrial production line, the freight logistics, etc.

Feature:

Safety, reliable in operation with minimum maintenance;

High effiency and small hand pull;

Light weight and easy handling;

Fine appearance with small size;

Durability in service.



==============
electric hoist accessories
https://www.liftingcn.com/accessories-of-electric-hoist/


When purchasing an electric hoist there are sometimes additional accessories required to make operation easier and more bespoke to your application. LES offer a huge range of electric hoist accessories such as radio control systems, festoon cable systems, transformers, weather jackets and much more. Browse our extensive range or contact our sales team for expert advice.

YALE ELECTRIC CHAIN HOIST SPARES & SPARE PARTS
 
RADIO CONTROL SYSTEMS
 
FESTOON CABLE SYSTEMS

RUNWAY BEAM END STOPS

--
Find out more about All Hoist Accessories from DLH Online
Niko Hoist Accessories
International brand Niko has a great reputation in the lifting and handling equipment industry for making lightweight cranes and crane accessories. As a popular producer of top-quality, versatile crane cables, jib cranes, scaffold runway systems and fall arrest tracks, Niko offers cost-effective and robust hoist accessories that are as easy to install as they are to use.

Our Niko Hoist Accessories include the highly recommended Twin C-rail Festoon Cable Supply and Remote Pendant Systems which will ensure a reliable power supply for electric chain hoists and organise cables for safer lifting. They are appreciated for their simple installation process and the fact that they are much more cost-effective than bus bars. If you find that a catenary taut wire cable festoon system is not ideal or practical for your work site, the Niko Twin C-rail Festoon Cable Supply will most likely do the trick. Because it is free-running in operation, this cable supply solution is extremely safe. Further, this solution is low-maintenance, making it popular for powering overhead electric hoists in both UK and international work sites. The comprehensive kit includes 2 track end stops, 2 end clamps. And 3-metre lengths of tracks. Support brackets are adjustable, giving you greater control over how you would like to get the job done.

We stock Niko NCL - 64amp 4-pole Enclosed Conductor Bar systems that will help you to power your electric hoist in a way that is secure and organised. Our Niko conductor bars will mean your workplace can be free of hanging cables because safety is a key feature of these singularly flexible and easy-to-install power supply solutions. The Niko NCL enclosed conductor bar system supports unhindered travel length, so there is no possibility of getting any cables bunched up at the feed end like with a festoon cable supply. A travel speed of up to 300 metres per minute depending on the application is a key advantage to the user.

At DLH Online we are happy to offer Niko Hoist accessories at a discount to our buyers, so you can start boosting efficiency and keep costs down at the same time.

Warrior Hoist Accessories
Warrior is a UK-based brand that is part of Winch Solutions Ltd. Warrior has been designing and supplying companies worldwide with hoists and related accessories for 14 years, so their hoist accessories are a staple of work sites around the globe.

Our Warrior Adjustable Length Rotary Hoist Arms with Scaffold Brackets have a maximum reach of between 750mm and 1100mm as well as a lifting capacity of 250 kg. They are compact, to save you space in the workplace, and are incredibly easy to install. For added strength and safety, they are fitted with special fixing clamps so that they stay in place when lifting. They are EN14492 compliant and perfect accessory for any of the Warrior electric scaffold hoists like in our DLH Online catalogue. Weighing only 6kg, Warrior Adjustable Length Rotary Hoist Arms with Scaffold Brackets are lightweight and easy to transport from one work site to another.

Here at DLH Online our friendly sales team are ready to help answer any questions you may have about how your electric hoist, manual hoist, pneumatic hoist or hoist accessories work. Should you need special controls or like any information about design and installation, we are keen to give you expert advice. We are also able to help you if you would like to know more about how your lifting and handling equipment will work in a special environment.

DLH Online is the main UK authorised distributor for Thern Inc., alongside being a top UK authorised distributor for the Columbus McKinnon Group (CMCO) who incorporate the Yale, Pfaff Silberblau, Steerman, and Camlok brands. DLH Online is also the Main UK-authorised distributor for Eepos, Schilling, Erikkila and Codipro. They are also the exclusive authorised Master UK distributors for Lifts All Sweden alongside being the key North West (UK) authorised distributors for Crosby, RUD and Donati and Sumner.

--

Electric hoists and accessories
Do you lift loads in your production facility several times a day and do you place great emphasis on process reliability, durability and workplace safety when you work with your lifting equipment?
If so, then we would be pleased to advise you on the correct choice of a suitable PLANETA electric hoist, quality products from flexible series production, designed in accordance with the most recent EC Machinery Directives.
Compact design, great ease of maintenance and long service life. Can be used for a vast array of lifting applications, as solo hoists, installed in a trolley or as a crane hoist. We offer load bearing capacities of up to 100 t as standard.
PLANETA electric hoists are in operation wherever process reliability is an important issue for the crane system. In gruelling three-shift operation in the automotive and other industries, in dusty or chemically aggressive environments, for external use, in the entertainments industry or for extreme lifting heights and speeds in wind power plants. Developed as standard for the most demanding of requirements:

Elektrokettenzüge1
Electric chain hoists
Elektroseilzuege5
Electric rope hoists
Elektrobauseilzuege9
Electric rope winch
E-Zug-Zubehör
Electric chain hoist / accessories
Stromzufuehrung5
Power supply

--
Hoisting Accessories
Quick Ref: CN-1237
Spring recoil power supply festoon cable reelers and cable reeling systems generally used on our range of electric hoists.
In this category we offer accessories for lifting hoists of all types. These accessories are to be used in conjunction with our hoists to make the lifting procedure easier and/or safer for the operator or those in the working area. Radio remote control means that the operator can get a clearer view of the hoisting path ensuring that the way ahead is always clear and the hoisting operation is safe. We produced power supply festoon systems for all hoists; electric chain hoists; Compressed air and hydraulic hoist. Our festoon system is trolleys that run in track or spring recoil power supply festoon systems. Other accessories include lifting baskets Lifting buckets, hosting wheel barrows and probably the most overloaded in this category being our LiftingSafety power converters. These unique products convert single phase eclectic supplies into 3Ph 415v which means that our customers can operate 3 phase electric lifting hoists when only a 230v single phase power supply is available. 

--
Hoists, Trolleys & Accessories
Make MSC your first choice for quality hoists, trolleys and accessories. We know that safety is your highest priority; that s why we stock a complete line of top brand electric, air and hand operated hoists to improve productivity in a multitude of material handling applications. You ll also find an extensive range of high capacity trolleys for fast and efficient transport of products. Whether you work in a warehouse, repair shop or a business that requires heavy lifting, MSC has the hoists, trolleys and accessories for your operation.
--



===============
electric hoist track
https://www.liftingcn.com/accessories-of-electric-hoist/c-rail/

https://www.model-engineer.co.uk/forums/postings.asp?th=107871   post
https://www.reddit.com/r/DIY/comments/1oaudy/electric_hoist_on_a_track_for_my_garage/  post

The Freeway TransactiveXtra Ceiling Track Hoist, exclusively manufactured by Prism Medical UK, is the safest, easiest and most practical way to safely transfer clients from one surface to another.

Installed at ceiling level, complete with innovative tracking solutions, the Freeway TransactiveXtra Ceiling Track Hoist provides the caregiver with increased access to the client – making their job safer, and making the transfer more comfortable for the client.

The TransactiveXtra benefits from a low profile design, which is unobtrusive – yet provides a much greater lifting height than any other hoist option.

With a range of track layouts available, advanced safety features and useful diagnostic tools, the TransactiveXtra can greatly improve quality of life for its users.

TransactiveXtra Models available
Maximum User Weight: 130kg (20.5 stone) with manual or powered traverse
Maximum User Weight: 160kg (25.2 stone) with manual or powered traverse
Maximum User Weight: 200kg (31.5 stone) with manual or powered traverse
Maximum User Weight: 270kg (42.5 stone) with manual or powered traverse
Please note: The price listed is for the hoist unit only. If you require a new hoist and track system, or wish to move an existing system, please contact us to organise a free no obligation survey.

--



==============
Electric Wire Rope Hoist
https://www.liftingcn.com/electric-hoist-and-winch/electric-wire-rope-hoist

CXT electric wire rope hoists
The CXT electric wire rope hoist is the most widely-used Konecranes product. Anywhere people want to lift up to 80 tons, you can often find a CXT hoist doing the job. The reliability and versatility of the CXT has made Konecranes the largest supplier of wire rope hoists in the world.

What do you want from your wire rope hoist?
Versatility means custom-tailored solutions for your every lifting need. Choose a normal headroom hoisting trolley when you have the space, or a low headroom model when you don't. Available in monorail or double girder models, flexibility is key. The CXT electric wire rope hoist adapts for the requirements of your runway and your building.

Do you need a swivel trolley for greater ease of movement? What about a fixed hoist, when movement is more restricted? The wire ropes are strong, highly flexible, and optimized to your specific reeving requirements. Tell us your needs, and we will give you a hoist to match them.

Konecranes also makes wire rope hoists for hazardous environments.

A wire rope hoist that lasts
Ideally, you should buy a full CXT crane, to ensure the quality of all of your lifting equipment. But if your budget is tight, you may wish to modernize your existing crane with the CXT hoist. Even if you only buy the hoist, we still service your whole crane, not just the Konecranes part.

Ensure your hoist stays safe and lasts longer with our unique TRUCONNECT® remote monitoring and reporting service. The condition monitoring unit on your hoist sends usage data to Konecranes. Periodic reports make it easy to manage safety, usage, and maintenance.
---
EUROBLOC VT ELECTRIC WIRE ROPE HOIST (VT1, VT2, VT3, VT4, VT5)
The Eurobloc VT electric wire rope hoist is a quality, heavy duty hoist best suited for high lifting capacities of 10,000kg or more and offers fast lifting speeds. The VT offers the smallest minimum hook height and hook approach distance on the market for a wire rope hoist, and there is also the possibility to adjust speed while travelling.

Galvanised steel wire rope with a high safety factor
Rotating hook and pulley block with safety latch
Improved motor cooling
Overload limiter as standard
MAKE AN ENQUIRY
Technical Information
Documents
Configurations
Related
Enquire
Catalogue
TECHNICAL INFORMATION
Verlinde’s new VT electric wire rope hoist has a lifting capacity from 800kg to 80,000kg and boasts a total of 13 patents for its market leading design.

Dual-speed hoisting motors with thermistor
DC disc brake, maintenance free (hoisting)
Four step geared limit switches
Electro-mechanical overload protection
Low voltage Control 48V
Standard power supplies are 380V/400V/415V/50Hz and 440V/460V/60Hz
IP55 / insulation class F motor protection
Push button box with emergency stop
Tropicalised motor for hoisting and travelling
Rope guide suitable for an aggressive environment
Time meter
EC Declaration of Conformity
Hook certificate
Steel wire rope certificate
Hoist owners manual according to EEC regulations
Set of electrical schematics

-
ELECTRIC WIRE ROPE HOISTS: 3 OPTIONS TO CHOOSE FROM
An Electric Wire Rope Hoist is a heavy duty lifting appliance with a higher lifting capacity than other hoisting options. Hoist UK offer three wire rope hoisting options that each have unique advantages and associated benefits and are each suited to different applications dependent on the user’s operation.

Our Electric Wire Rope Hoist options include VT Electric Wire Rope Hoist.
VM Essentials Electric Wire Rope Hoists (for use with crane kits only),
VT Open Barrel Electric Wire Rope Hoist.
-
WIRE ROPE HOISTS VS. CHAIN HOISTS
Both wire rope hoists wire rope hoists and chain hoists are robust lifting appliances that are widely used across numerous industry sectors in a variety of lifting applications. Wire rope hoists have higher lifting capacities and our range of Eurobloc VT electric wire rope hoists are able to lift up to 250 tonnes, compared with 10 tonnes from our electric chain hoists and 50 tonnes from our manual chain hoists. The greater lifting capacity is one of the factors that makes wire rope hoists a more expensive option compared with a chain hoist, but there are other things to consider when trying to decide whether a wire rope hoist or a chain hoist would be better suited to your operation.
-
ACHIEVING TRUE VERTICAL LIFT FOR PRECISE LIFTING WITH A WIRE ROPE HOIST
In essence, true vertical lift is a hoists ability to lift the hook straight up and down, to pick up or put down a load in an exact position with no hook drift. It occurs when a hoist (lower block) moves in a true vertical path between the lower limit of travel, which happens when the rope(s) anchored at each end of the drum wind from the centre of the drum outward (inward when raising the hook); enabling the hook and load to be centred below the middle of the drum. This design prevents the hook from wandering from one end of the drum to the other in the highest and lowest hook positions.
-
---

Electric Wire Rope Hoists, Wire Rope Hoist, Electric Rope Hoist
In lifting equipment crane, there has been applied in different sites widely, such as cable reel equipment, transportation, hoist and crane etc. Nowadays the application has been expanding to other industries. There are several types of crane : fixed crane, mobile crane, derrick, elevator, construction lifter and cage lift, etc... and we have been receiving orders from South Africa markets and used in Chemical industry. We welcome worldwide buyers to contact us and we look forward to your inquiry!

Our electric wire rope hoist (electric rope hoist) has been widely applied to lifting facility, crane, and with features are below:

Our hoist uses the wire rope of the intermediate intensity. Though the overall size is greater than the hoist with high intensity wire rope, it’s excellent to absorb energy when load impact repeatedly. Thus, it can extend fatigue time. Further, larger contact area of wire rope, lower the abrasion rate. More, it’s easy to buy this type of wire rope, you can lower the maintenance cost.
Reducer and electric motor are located at two sides of drum. Transmission via drive shaft which is inside of the drum. The device is conducive to the balance of traversing and solves the balance problem as well.
Our wire rope hoist frame is built out of weld formed frame is built out of weld formed before processing that is with higher impact resistance compared to bolted joint type.
Two selections for brake: AC & DC to meet market demand.
For Hoist with smaller trolley gauge, shaft for traversing wheel can be adjusted according to the height. It can match up the error of two girder cambers and ensures four wheels touching the traversing rail.
The main electric components are adopted from well-known brands, and easy to purchase.
Why AC (Alternating Current) or DC (Direct Current) Brakes?

Both of AC and DC can comply with industrial requirement which using in our electric wire rope hoists very well. Unless you have specific considering about “Noise level”, DC Brake should be good choice.
AC : 90~100 db , DC : 70~80 db
We use INTORQ (Lenze Germany) DC Electromagnetic safety brake. Besides low noise basic request, it’s with big brake torque, long life span. Its features come from multi-coil technology instead of the single structure, as well as wear-resistant rotor capability to achieve the torque requirements for users. The brake reaction speed becomes one of key points to users, if the brake doesn’t open in time, will make the motor blocked and burned. INTORQ has good solution on this.

---

WIRE ROPE HOISTS
ABUS electric wire rope hoists are the core element of our crane systems. They are also the result of many decades of research and development by ABUS. Our wire rope hoists are produced at the ABUS production plants at Gummersbach using the most advanced technology available and continue to bear witness to the reliability, and durability of our products. The SWL range of ABUS electric wire rope hoists extends from 1 t to 120 t. Our customers can choose from a wide range of models depending on application and requirements - starting with the standard wire rope hoist in the lower SWL range up to special crab unit designs incorporating additional features at the higher SWL range. However, all wire rope hoists have these characteristics in common: highest levels of uptime availability and safety within materials handling operations.

---


===============
Electric Chain Hoist
https://www.liftingcn.com/electric-hoist-and-winch/electric-chain-hoist/

I bought the automatic electric hoist for my farm and my shop, I raise the hay bales by means of the hoist. The construction of this tool is very solid, and I can happily say that this one is more beneficial than 220/440 lb. capacity (I made some research before buying this one). And this hoist has 440/880 lb capacity.
The general operation is rather smooth, but I can tell that stops and starts are sudden and rough. It has positive brake, it does not let the cable slip. It also has overlimit device, and its construction is not plastic, it is steel. The cord of the operating switch is about 6 feet, it is enough for me, but if you want longer, you should wire it with the help of the conductor.

Be attentive when you lift any load, it should be straight, so that the cable wraps properly. If the cable is often bunched up on one side, and you often lift heavy loads, you may face a rather fast wearing out of the cable. So take this into account.

It has the instructions, and it is rather clear. The operation of the device is smooth and sure. The finish is nice. By the way, the hanger loops fit PL-1000 Unistrut type.

In general, this tool does its job well. It is a very good assistant.

Check the price
What is the difference between winches and electric hoists?
In fact, their operation is similar, however there are still some significant differences. One of the differences is braking system, it acts in a different way. So you should take it into account while selecting between these tools. Jeeps and also 4×4 vehicles have winches with the dynamic braking system, i.e. the resistance in the gears of the winch is used to hold loads. This version does not work for suspended load, otherwise it may lead to stripped gears, and as a result of it, the load may be dropped.

As to the electric hoist, a mechanical braking system is used, i.e. the suspended payload is fixed in place by means of the physical brake (not hoist gears). It provides a good protection of the lift gears, and the line bleed is also prevented.

A free-spool mechanism is not provided at the electric hoists. And this is another difference between these tools. Winches just require this mechanism, so that the button should not be hold in order to extend the winch line for better spooling out and attaching the cable. Also, winches go without the free-spooling option in order to reduce a risk of the accidental dropping of the load. Some electric hoists are equipped with a switch to cut off the hoist in case of lifting a payload weighing more than it can hold.

Moreover, there are electric winch that could be designed as a hoist. To have this option, the free-spool option should be removed (or disabled), and the brake system should be locked without the gears. Be attentive and always check whether your device have the double duty as a hoist. In other cases, you must not use it because it is dangerous for an operator.

Mounting Options for Electric Hoist
The industrial electric hoists set up with different mounting options, so that it can be used in different ways. Lug mounted, hook suspension, and lug mounted are the most common. The uncommon custom setups may be also found, if it is needed.

In case of the trolley mounted hoists, it is placed on a track, or an i-beam. The hoist is fixed, and so any point is available (along the rail or beam).

The lug mount configuration is used in the electric hoist that is mounted with bolt holes attached to threaded lugs. There are also lug mounts with trolley system.

A suspension hook mount hoists use a hook on top of the unit attached to the mated hook hanging from the ceiling. During the installation, the support for your hoist and loads should be really strong to keep that load. In order to prevent accidents during the use of the device, make sure to use strong mounts, hoists, and supports that are solid.

--

Single Phase Electric Hoists (110V & 240V)
Our Electric Lifting Hoists are the perfect piece of equipment to assist lifting applications where a manual hoist is not enough. Available both to buy and hire, our Electric Chain Hoist collection can be used to lift loads of up to 1 tonne - each Electric Hoist has a different weight limit, so please be sure to check this before making your selection.

SafetyLiftinGear's single phase Electric Chain Hoists are available in both 110V and 240V configurations. Browse our entire Electric Hoist range below:

--
Electric Chain Hoists
Quick Ref: CN-6
Discounted high quality, low cost electric chain blocks (chain hoists) - We can supply an electrically powered hoist to suit almost any budget and application.
LiftingSafety offer in our online shop/catalogue a range of Electric chain hoists to suit most applications from many of the leading quality hoist manufacturers including Yale, RWM, Donati, Tractel, Verlinde, Kito and many more to come in the near future. We are constantly looking for new manufacturers with additional lifting equipment features so that we will be able to cater for all our customers requirements.

Options for the powered chain hoists that we offer are very similar to that of the manual hand chain hoist with the addition of powered motions as opposed to requiring manual effort to raise or travel the load along the manorial beam.

Our electric lifting hoists are fitted with supplied hook suspension or with an integrated manual or powered trolley and they can be controlled by a push button pendant or by radio remote control. Options are available with slow, fast or variable lifting speeds and hoists can be supplied in voltages (power supplies) and bespoke hoists suitable for different environments dependant on our user requirements.

We can also supply specialist application units which have been specifically designed for use on wind turbines and Atex areas. We appreciate that an electrically driven chain hoist can represent a sizable investment and so if you are even a little unsure as to the most appropriate model then please contact our sales or technical staff who will assist you accordingly.

-

More Information
An electric hoist, with a mains powered electric motor (generally 110v, 240v or 415v DC) and that utilises a chain to perform the lift, is often referred to by a more common term which is an 'electric chain hoist'. We can supply almost any type or brand of electric hoist from most major hoisting equipment manufacturers. We are also a supplier of a complete range of manual chain hoists, wire rope hoists and scaffold hoists that could possibly prove to be a better suited hoist for the more specific application.

Just about all of the hoists which we supply are also available with a full range of customisations and accessories to suit, which can add usability, practicality and functionality, that then in turn can ease user effort required, thus increasing productivity and possibly reducing overall production costs.

This particular type of hoisting equipment can be supplied with a variety of compatible options such as:

1Ph (single phase) electric - Generally 110v or 230v/240v
3Ph (three phase) electric - Industrial 400v/415v
Capacities ranging from 60kg up to 50000kg.
Wide range of other unit specific features such as twin hooks or spark resistance for example.
Note: One of our electric winches may also be a more suitable lifting device, which could make lifting and handling your loads easier, more efficient, and possibly faster. Also available, which may be of interest is a wide range of air hoists, which have a more specific assortment of features, that make them more suitable for conditions such as hazardous environments or under-water (sub-sea) for example.

---

Up to 5.000 kg of lasting lifting power
Konecranes offers three electric chain hoists designed for flexibility and durability in lifting. The Konecranes C-series electric chain hoist and the CLX electric chain hoist can lift up to 5.000 kg, whereas SLX electric chain hoist can take up to 2.500 kg, giving you the versatility you need in industrial applications and at demanding workstations.

Compact headroom, hook suspension and a range of other features make our hoists easily adjustable for your specific workstation needs.

 

Visit the dedicated website for Konecranes C-series!
Visit the dedicated website for CLX!
 

Efficiency and safety in the same package
The new Konecranes C-series is our most advanced electrical chain hoist to date. Thoroughly redesigned from inside out for over a million operations, Konecranes C-series electric chain hoist combines usability, enhanced performance and durability for real lifecycle value.

Easy to use, the CLX electric chain hoist can speed up work cycles, enhance safety and extend service life. Adaptable and long-lasting, it is ideal for any busy workstation.

Choose the SLX electric chain hoist with stepless hoisting speeds for smooth vertical movement, keeping your load steady throughout the most demanding workloads. It has all the CLX features and more, such as an electronic overload protection, slack chain control, and shock load absorption. It combines efficiency and safety with its advanced technology.

Lift almost anywhere
You can use these electric chain hoists on an overhead crane, a workstation crane, or with a jib crane. Their versatility makes Konecranes electric chain hoists an ideal solution for many lifting applications.

Read more about the Konecranes C-series electric chain hoist on our dedicated website at konecranes.com /newseries/c-series or about CLX and SLX hoists on our dedicated website at konecranes.com/clx. Contact us today for more information.

 ---
ELECTRIC CHAIN HOISTS (3 PHASE)
Powered Chain Hoists with Powered and Manual Trolleys
Hoist UK supply a variety of Electric Chain Hoists and Trolleys from leading international lifting equipment manufacturer Verlinde. Our high quality electric chain hoists are capable of lifting loads from 63kg to 10 tonnes and we offer a range of electric, manual and geared trolleys, including trolleys for curved beams and low headroom working environments.

Not sure whether you need an Electric Chain Hoist or an Electric Wire Rope Hoist? Read our focus piece comparing the two: Wire Rope Hoists VS. Electric Chain Hoists.
-

DO YOU NEED THE POWER OF AN ELECTRIC WIRE ROPE HOIST WITHOUT THE COST?
The VM Essentials Wire Rope Hoist has been designed for use with crane kits, giving you the power of an electric wire rope hoist without the cost. With a lifting capacity of 2,000kg to 20,000kg, the VM Essentials is controlled by pendant or radio control and unlike the VT electric wire rope hoist it's optimised for use on an overhead/underslung crane.

-
OUR PRODUCTS
Hoist UK supplies a wide range of compact electric chain hoists for use in industrial environments and are also available to offer additional options for bespoke applications. Our range includes hoists with hook suspension, powered, manual and much more.

Our electric chain hoists can be operated by either a simple push button control or radio remote control and come as standard with dual lifting speeds, but if a higher level of precision is required, we can offer variable speed lifting with Extended Speed Range (ESR) which allows you to optimize the speed of your hoist. The voltage for the standard range of our electric chain hoists is 400V / 3Ph / 50hz, but other voltages are available on request.

Using a powered chain hoist will reduce the risk of injury on the person lifting the heavy load, and Hoist UK can supply a range of complimentary products to assist with your specific lifting application such as jib cranes, mobile gantries or an overhead crane. Electric chain hoists are common in a variety of workplaces, they are easy to use and are a valuable tool enabling loads to be lifted quickly and safely.
-
WHEN DOES YOUR HOIST NEED A GENERAL OVERHAUL OR TO BE REPLACED?
Hoists, whether they are electric chain hoists, manual chain hoists, electric wire rope hoists or electric belt hoists are all manufactured with 10 years of serviceable life before a major overhaul or replacement is required. The ten year service life may not necessarily be a physical ten years of operation, but may be used up more quickly or slowly based on how the machine is being operated during its working life.

In order to help evaluate the working life of a hoist you need to be able to calculate how much of the original manufacturers Safe Working Period exists after your lifting operations have occurred.

READ MORE

TRAINS COMPONENT ASSEMBLY, UK
A manufacturer of train components with on-site assembly operations required a motorised crane system for safe and easy management of large, heavy parts and materials during the process.

It was very important that the customer didn't lose any production time so the installation was planned for a weekend to ensure minimal disruption to their operations.

Our team of lifting engineers worked around the clock to ensure the installation and testing was completed during the designated weekend, leaving enough time for some user training before the system became operational on the Monday morning.

---
ELECTRIC CHAIN HOISTS
Our fantastic range of Eeectric chain hoists is offered by Columbus Mckinnon and Stahl. Yale’s extensive variety of unmatched quality hoists is also supplied. We provide amazing discounts on our entire range of electric hoists including industry leading prices on the Yale Cps electric chain hoist.

Electric Chain Hoist Suitable for Lifting Heavy Materials
Our range of electric chain hoists easily hook to scaffolding and allow the task of lifting building materials task simple when lifting between floors or to upper storeys and roofs. They are perfect for attaching to beams and scaffolding, sometimes requiring an accompanying beam clamp or trolley. Moreover, chain hoists are manufactured with a guide, ensuring a flawless lift.

Tough loads like building materials and heavy engines are easily lifted to their intended locations. For this purpose, electric hoists are the perfect choice. They are of a solid steel construction with a powder coating to help prevent corrosion and ensure an aesthetically pleasing finish. Powder coated products also possess excellent scratch resistance. For both static and dynamic loading, these hoist come complete with internal brakes. Some hoists have an externally adjustable slip clutch creating a connection between the brake and the load.

-
Electric Scaffold Hoist
Scaffold hoists are very versatile pieces of lifting equipment which are used in several industries. Scaffolding wire rope hoists are those hoists that are made specifically for lifting building materials and tools from the ground to the working area above. Scaffold hoists are the perfect choice for building sites and are also known as wire rope lifting hoist. They are suitable for outdoor use and equipped with a bracket and clasps which can be attached to a scaffold tower.

Scaffold hoists possess fast lifting speed and usually have an extended height of lift to help reach your working platform from the floor. Lifting speed is crucial to saving time and money.

Contact Us for Your Requirements
If you want a product which you do not see listed then simply call us on 029 2046 5988 or send an email to info@bishopliftingequipment.co.uk. Our hospitable sales staff will be delighted to help you. Bishop have the right electric chain hoists for all your lifting needs no matter what Working Load Limit, i.e WLL.

---
ELECTRIC CHAINHOIST
These powered lifting machines are ideal for use on an industrial or construction projects that require the lifting of heavy duty loads.
By operating the machine via a remote control users can ensure they can work the electric chain block from a safe distance.
The Safe Working Load (SWL) for the electric chain hoist ranges from 250kg to 10 tonnes and a variety of different heights of lift,
chain and pendant control are available so you can choose the correct specifics depending on the requirements of your job.
Available in a plethora of voltages including 110v, 240v and 415v, the electric chain hoists are also equipped with a low voltage pendant.
This easy to assemble hoist is perfect for minimising risk when moving heavy loads