### You are here:

# Bright silver reflective thermal film

PES
Reflection coefficient: greater than 400CPL

Washing performance: 25 washes at 60 ℃ (ISO6330)

ENISO20471 ANSI107 OEKO-TEX100

- Previous
- Next

Description
Related Products

##### Bright silver diagonal reflective thermal film

##### High gloss engraved reflective thermal film

##### Colorful Hot Post

##### Bright silver reflective flame-retardant cloth

##### Reflective synthetic fabric

##### Grey high gloss synthetic fiber-2A reflective cloth

##### Grey reflective strip

##### Reflective stripe