### You are here:

# High gloss engraved reflective thermal film

PES
Reflection coefficient: greater than 230CPL

Washing performance: 25 washes at 40 ℃

ENISO20471 ANSI107 OEKO-TEX100

- Previous
- Next

Description
Related Products

##### Colorful Hot Post

##### Bright silver reflective flame-retardant cloth

##### Fluorescent yellow flame retardant cloth warning tape

##### Bright silver double-sided elastic fabric

##### Bright silver diagonal reflective thermal film

##### Bright silver reflective thermal film

##### Reflective synthetic fabric

##### Grey high gloss synthetic fiber-2A reflective cloth