Products

## Lock Cylinder

Euro Mortise Lock
Impotent Features & Benefits l Conforms to the requirements of EN12209-3 l Single or triple deadbolts with one or two throws. l Quick reversible latch for easy on-site handing. l Reversible latch bolts can be optioned to be operating by key or handle. l 3point latch to enable smooth and quite closing . Also can prevent door from slamming. l Adjustable roller latch l Hook latch for steel door or pull gate l Large range of cylinders conforming to EN1303 with various features. l The KA and MK/GMK are available Face plate l Material: Stainless steel 201 304 316 l Type: round head / square head l Thickness: 3mm l Width: 22mm l Finish: SS/SP/AB/AC/ PVD Striker plate: l Material: Stainless steel 201 304 316 l 1.2mm thickness, 1.5mm available l Finish: SS/SP/AB/AC/ PVD Lock case l Material: Steel, 1.2mm thickness l Electrolysis board/Yellow crackle/Silver board/Black crackle/ Snow-flake board.