Products

## CL01.01: Double straight bolt

<<Previous Next>>

Description:
· Single turn, 3 pins cylinder lock
· Interchangeable: With most common roller shutter locks available on the market. The reinforced bolt makes the roller shutter more resistant to attack.
· Available for motorized roller shutter
· Reinforced steel bolt: 2mm steel plated folded back on itself to reach overall 6.5mm thickness
· Straight, shifted, Lengthened bolt available with 6mm hole
· Solid brass cylinder
· Rustproof zinc plated box and components
· 3 brass key, chromed plated

Item No. | A | B | PINS | FINISH | QTY/BOX
CL01.01 | 155 | 56 | 3 | GALVANIZED | 6